{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["งานฐานราก","รายการคำนวณเสา"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"งานฐานราก","index":0,"n_rows":26,"n_cols":141,"rows_kept":26,"cut":false,"hidden":false,"merged":[[0,1,0,2],[4,22,4,23],[4,26,4,27],[4,30,4,31],[3,1,3,2],[3,3,3,5],[3,6,3,8],[3,18,3,19],[3,16,3,17],[3,12,3,14],[3,9,3,10],[3,21,3,24],[3,25,3,28],[3,29,3,32],[2,34,2,35],[2,21,2,32],[2,11,2,15],[2,1,2,10],[2,16,2,20],[5,44,7,44],[4,40,4,41],[3,39,3,42],[2,36,2,42],[3,36,3,38],[4,44,4,45],[3,44,3,45],[5,63,7,63],[5,48,7,48],[5,49,7,49],[5,47,7,47],[5,45,7,45],[5,46,7,46],[5,64,7,64],[5,65,7,65],[5,67,7,67],[5,66,7,66],[5,68,7,68],[4,67,4,68],[4,65,4,66],[3,65,3,66],[3,67,3,68],[2,44,2,68],[4,46,4,47],[4,48,4,49],[3,63,3,64],[4,63,4,64],[3,50,3,62],[3,48,3,49],[3,46,3,47]]}
[null,"ประมาณงานฐานราก",null,null,"(เป็นการคำนวณหาปริมาตร และ ปริมาณ)",null,null,"โดย","นาย ปรีชา สุนทรภักดี"]
[]
[null,"งานคอนกรีต",null,null,null,null,null,null,null,null,null,"งานดินขุด",null,null,null,null,"งานดินถม",null,null,null,null,"งานเหล็กฐานราก",null,null,null,null,null,null,null,null,null,null,null,"งานแบบฐานราก","งานเสาเข็ม",null,"งานเหล็กตอม่อ",null,null,null,null,null,null,null,"สรุป : รวมปริมาณงานฐานราก"]
[null,"รายการ",null,"ขนาดเสาตอม่อ",null,null,"ขนาดฐานราก",null,null,"รวมปริมาณคอนกรีต",null,"ชนิดของดิน","ขนาดหลุม",null,null,"รวมปริมาณดินขุด","คอนกรีตหยาบ",null,"ทรายหยาบ ",null,"รวม","เหล็กเสริมตาม กว้าง",null,null,null,"เหล็กเสริมตามยาว",null,null,null,"เหล็กปลอก (รัดรอบ)",null,null,null,null,null,null,"เหล็กยืน",null,null,"เหล็กปลอก",null,null,null,null,"ปริมาตรคอนกรีต",null,"ปริมาตรดินขุด",null,"ปริมาตรดินถม",null,"งานเหล็ก",null,null,null,null,null,null,null,null,null,null,null,null,"งานแบบฐาน",null,"คอนกรีตหยาบ",null,"ทรายหยาบ"]
["No.","ลำดับที่","ชื่อ","กว้าง (ม.)","ยาว (ม.)","สูง (ม.)","กว้าง (ม.)","ยาว (ม.)","สูง (ม.)","จำนวน","รวม (ม.3)","เลือก","กว้าง (ม.)","ยาว ( ม.)","สูง (ม.)","รวม (ม.3)","หนา","รวม.","หนา","รวม.","รวม (ม.3)","ขนาดเหล็กเสริมø","ระยะห่าง (ม.)",null,"รวม( ม.)","ขนาดเหล็กเสริมø","ระยะห่าง (ม.)",null,"รวม (ม.)","ขนาดเหล็กเสริมø","ระยะห่าง (ม.)",null,"รวม (ม.)","   รวม (ม.2)","จำนวน","รวม (ต้น)","จำนวน (ท่อน)","ขนาดø","รวม (ม.)","ขนาดø","ระยะห่าง",null,"รวม (ม.)",null,"รวม",null,"รวม",null,"รวม",null,"RB6","RB9","RB12","RB15","RB19","RB25","DB12","DB16","DB20","DB25","DB28","DB32","หน่วย","รวม.",null,"รวม",null,"รวม"]
[null,1,"F1-1",0.1,0.1,null,null,null,null,null,{"$f":"(D6*E6*F6+G6*H6*I6)*J6","v":0},"ดินแข็ง",{"$f":"G6","v":0},0,null,{"$f":"ROUND(IF(AND(L6=\"ดินแข็ง\",O6<=1.5),((M6+0.2*2)*(N6+0.2*2))*O6,IF(AND(L6=\"ดินแข็ง\",O6>1.5),((M6+0.3*2)+(N6+0.3*2))*O6,IF(AND(O6<=1.5,L6=\"ดินอ่อน\"),1/3*O6*(((N6+0.2*2)*(M6+0.2*2))+((N6+0.3*O6*2)*(M6+0.3*O6*2))+SQRT((((N6+0.2*2)*(M6+0.2*2))*((N6+0.3*O6*2)*(M6+0.3*O6*2))))),IF(AND(O6>1.5,L6=\"ดินอ่อน\"),1/3*O6*(((N6+0.3*2)*(M6+0.3*2))+((N6+0.5*O6*2)*(M6+0.5*O6*2))+SQRT((((N6+0.3*2)*(M6+0.3*2))*((N6+0.5*O6*2)*(M6+0.5*O6*2))))))))),2)*J6","v":0},null,{"$f":"ROUND(IF(AND(L6=\"ดินอ่อน\",O6>1.5),(((G6+0.3*2)*(H6+0.3*2))*Q6),IF(AND(L6=\"ดินอ่อน\",O6<=1.5),(((G6+0.2*2)*(H6+0.2*2))*Q6),IF(AND(L6=\"ดินแข็ง\",O6<=1.5),(((G6+0.2*2)*(H6+0.2*2))*Q6),IF(AND(L6=\"ดินแข็ง\",O6>1.5),(((G6+0.3*2)*(H6+0.3*2))*Q6))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L6=\"ดินอ่อน\",O6>1.5),(((G6+0.3*2)*(H6+0.3*2))*S6),IF(AND(L6=\"ดินอ่อน\",O6<=1.5),(((G6+0.2*2)*(H6+0.2*2))*S6),IF(AND(L6=\"ดินแข็ง\",O6<=1.5),(((G6+0.2*2)*(H6+0.2*2))*S6),IF(AND(L6=\"ดินแข็ง\",O6>1.5),(((G6+0.3*2)*(H6+0.3*2))*S6))))),3)","v":0},{"$f":"P6-K6+T6+R6","v":0},"RB 12 mm.","@",null,{"$f":"IF(X6=0,0,((G6/X6)+1)*(H6+(I6*2))*J6)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB6=0,0,((H6/AB6+1)*(G6+I6*2))*J6)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF6=0,0,((I6/AF6+1)*(H6*2+G6*2))*J6)","v":0},{"$f":"(G6*I6*2)+(H6*I6*2)+(D6*F6*2)+(E6*F6*2)","v":0},null,{"$f":"J6*AI6","v":0},null,"RB 12 mm.",{"$f":"IF(F6=0,0,F6+(G6/3))*AK6","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP6=0,0,(ROUNDUP(F6/AP6+1,0)*(D6*2+E6*2))*AK6)","v":0},null,{"$f":"SUM(K6:K25)","v":0},"ม3.",{"$f":"SUM(P6:P26)","v":0},"ม3.",{"$f":"SUM(U6:U26)","v":0},"ม3.",{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"RB 6 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"RB 9 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"RB 12 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"RB 15 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"RB 19 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"RB 25 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"DB 12 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"DB 16 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"DB 20 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"DB 25 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"RB 28 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},{"$f":"SUMIF(V6:V26:Z6:Z26:AD6:AD26:AL6:AL26:AN6:AN26,\"DB 32 mm.\",Y6:Y26:AC6:AC26:AG6:AG26:AM6:AM26:AQ6:AQ26)","v":0},"ม.",{"$f":"SUM(AH6:AH26)","v":0},"ม.2",{"$f":"SUM(R6:R26)","v":0},"ม.3",{"$f":"SUM(T6:T26)","v":0},"ม.3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(DH6*DJ6*2)+(DI6*DJ6*2)+(DE6*DG6*2)+(DF6*DG6*2)","v":0},6,{"$f":"DK6*EJ6","v":0}]
[null,2,"F1-2",0.1,0.1,null,null,null,null,null,{"$f":"(D7*E7*F7+G7*H7*I7)*J7","v":0},"ดินแข็ง",{"$f":"G7","v":0},{"$f":"H7","v":0},null,{"$f":"ROUND(IF(AND(L7=\"ดินแข็ง\",O7<=1.5),((M7+0.2*2)*(N7+0.2*2))*O7,IF(AND(L7=\"ดินแข็ง\",O7>1.5),((M7+0.3*2)+(N7+0.3*2))*O7,IF(AND(O7<=1.5,L7=\"ดินอ่อน\"),1/3*O7*(((N7+0.2*2)*(M7+0.2*2))+((N7+0.3*O7*2)*(M7+0.3*O7*2))+SQRT((((N7+0.2*2)*(M7+0.2*2))*((N7+0.3*O7*2)*(M7+0.3*O7*2))))),IF(AND(O7>1.5,L7=\"ดินอ่อน\"),1/3*O7*(((N7+0.3*2)*(M7+0.3*2))+((N7+0.5*O7*2)*(M7+0.5*O7*2))+SQRT((((N7+0.3*2)*(M7+0.3*2))*((N7+0.5*O7*2)*(M7+0.5*O7*2))))))))),2)*J7","v":0},null,{"$f":"ROUND(IF(AND(L7=\"ดินอ่อน\",O7>1.5),(((G7+0.3*2)*(H7+0.3*2))*Q7),IF(AND(L7=\"ดินอ่อน\",O7<=1.5),(((G7+0.2*2)*(H7+0.2*2))*Q7),IF(AND(L7=\"ดินแข็ง\",O7<=1.5),(((G7+0.2*2)*(H7+0.2*2))*Q7),IF(AND(L7=\"ดินแข็ง\",O7>1.5),(((G7+0.3*2)*(H7+0.3*2))*Q7))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L7=\"ดินอ่อน\",O7>1.5),(((G7+0.3*2)*(H7+0.3*2))*S7),IF(AND(L7=\"ดินอ่อน\",O7<=1.5),(((G7+0.2*2)*(H7+0.2*2))*S7),IF(AND(L7=\"ดินแข็ง\",O7<=1.5),(((G7+0.2*2)*(H7+0.2*2))*S7),IF(AND(L7=\"ดินแข็ง\",O7>1.5),(((G7+0.3*2)*(H7+0.3*2))*S7))))),3)","v":0},{"$f":"P7-K7+T7+R7","v":0},"RB 12 mm.","@",null,{"$f":"IF(X7=0,0,((G7/X7)+1)*(H7+(I7*2))*J7)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB7=0,0,((H7/AB7+1)*(G7+I7*2))*J7)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF7=0,0,((I7/AF7+1)*(H7*2+G7*2))*J7)","v":0},{"$f":"(G7*I7*2)+(H7*I7*2)+(D7*F7*2)+(E7*F7*2)","v":0},null,{"$f":"J7*AI7","v":0},null,"RB 12 mm.",{"$f":"IF(F7=0,0,F7+(G7/3))*AK7","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP7=0,0,(ROUNDUP(F7/AP7+1,0)*(D7*2+E7*2))*AK7)","v":0},null,null,null,null,null,null,null,{"$f":"AY6*0.22","v":0},{"$f":"AZ6*0.5","v":0},{"$f":"BA6*0.89","v":0},{"$f":"BB6*1.39","v":0},{"$f":"BC6*2.23","v":0},{"$f":"BD6*3.58","v":0},{"$f":"BE6*0.89","v":0},{"$f":"BF6*1.58","v":0},{"$f":"BG6*2.47","v":0},{"$f":"BH6*3.58","v":0},{"$f":"BI6*4.83","v":0},{"$f":"BJ6*6.31","v":0},"ก.ก."]
[null,3,"F1-3",0.1,0.1,null,null,null,null,null,{"$f":"(D8*E8*F8+G8*H8*I8)*J8","v":0},"ดินแข็ง",{"$f":"G8","v":0},{"$f":"H8","v":0},null,{"$f":"ROUND(IF(AND(L8=\"ดินแข็ง\",O8<=1.5),((M8+0.2*2)*(N8+0.2*2))*O8,IF(AND(L8=\"ดินแข็ง\",O8>1.5),((M8+0.3*2)+(N8+0.3*2))*O8,IF(AND(O8<=1.5,L8=\"ดินอ่อน\"),1/3*O8*(((N8+0.2*2)*(M8+0.2*2))+((N8+0.3*O8*2)*(M8+0.3*O8*2))+SQRT((((N8+0.2*2)*(M8+0.2*2))*((N8+0.3*O8*2)*(M8+0.3*O8*2))))),IF(AND(O8>1.5,L8=\"ดินอ่อน\"),1/3*O8*(((N8+0.3*2)*(M8+0.3*2))+((N8+0.5*O8*2)*(M8+0.5*O8*2))+SQRT((((N8+0.3*2)*(M8+0.3*2))*((N8+0.5*O8*2)*(M8+0.5*O8*2))))))))),2)*J8","v":0},null,{"$f":"ROUND(IF(AND(L8=\"ดินอ่อน\",O8>1.5),(((G8+0.3*2)*(H8+0.3*2))*Q8),IF(AND(L8=\"ดินอ่อน\",O8<=1.5),(((G8+0.2*2)*(H8+0.2*2))*Q8),IF(AND(L8=\"ดินแข็ง\",O8<=1.5),(((G8+0.2*2)*(H8+0.2*2))*Q8),IF(AND(L8=\"ดินแข็ง\",O8>1.5),(((G8+0.3*2)*(H8+0.3*2))*Q8))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L8=\"ดินอ่อน\",O8>1.5),(((G8+0.3*2)*(H8+0.3*2))*S8),IF(AND(L8=\"ดินอ่อน\",O8<=1.5),(((G8+0.2*2)*(H8+0.2*2))*S8),IF(AND(L8=\"ดินแข็ง\",O8<=1.5),(((G8+0.2*2)*(H8+0.2*2))*S8),IF(AND(L8=\"ดินแข็ง\",O8>1.5),(((G8+0.3*2)*(H8+0.3*2))*S8))))),3)","v":0},{"$f":"P8-K8+T8+R8","v":0},"RB 12 mm.","@",null,{"$f":"IF(X8=0,0,((G8/X8)+1)*(H8+(I8*2))*J8)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB8=0,0,((H8/AB8+1)*(G8+I8*2))*J8)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF8=0,0,((I8/AF8+1)*(H8*2+G8*2))*J8)","v":0},{"$f":"(G8*I8*2)+(H8*I8*2)+(D8*F8*2)+(E8*F8*2)","v":0},null,{"$f":"J8*AI8","v":0},null,"RB 12 mm.",{"$f":"IF(F8=0,0,F8+(G8/3))*AK8","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP8=0,0,(ROUNDUP(F8/AP8+1,0)*(D8*2+E8*2))*AK8)","v":0},null,null,null,null,null,null,null,{"$f":"ROUNDUP((AY6/10),0)","v":0},{"$f":"ROUNDUP((AZ6/10),0)","v":0},0,0,0,0,0,0,0,0,0,0,"เส้น"]
[null,4,"F1-4",0.1,0.1,null,null,null,null,null,{"$f":"(D9*E9*F9+G9*H9*I9)*J9","v":0},"ดินแข็ง",{"$f":"G9","v":0},{"$f":"H9","v":0},null,{"$f":"ROUND(IF(AND(L9=\"ดินแข็ง\",O9<=1.5),((M9+0.2*2)*(N9+0.2*2))*O9,IF(AND(L9=\"ดินแข็ง\",O9>1.5),((M9+0.3*2)+(N9+0.3*2))*O9,IF(AND(O9<=1.5,L9=\"ดินอ่อน\"),1/3*O9*(((N9+0.2*2)*(M9+0.2*2))+((N9+0.3*O9*2)*(M9+0.3*O9*2))+SQRT((((N9+0.2*2)*(M9+0.2*2))*((N9+0.3*O9*2)*(M9+0.3*O9*2))))),IF(AND(O9>1.5,L9=\"ดินอ่อน\"),1/3*O9*(((N9+0.3*2)*(M9+0.3*2))+((N9+0.5*O9*2)*(M9+0.5*O9*2))+SQRT((((N9+0.3*2)*(M9+0.3*2))*((N9+0.5*O9*2)*(M9+0.5*O9*2))))))))),2)*J9","v":0},null,{"$f":"ROUND(IF(AND(L9=\"ดินอ่อน\",O9>1.5),(((G9+0.3*2)*(H9+0.3*2))*Q9),IF(AND(L9=\"ดินอ่อน\",O9<=1.5),(((G9+0.2*2)*(H9+0.2*2))*Q9),IF(AND(L9=\"ดินแข็ง\",O9<=1.5),(((G9+0.2*2)*(H9+0.2*2))*Q9),IF(AND(L9=\"ดินแข็ง\",O9>1.5),(((G9+0.3*2)*(H9+0.3*2))*Q9))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L9=\"ดินอ่อน\",O9>1.5),(((G9+0.3*2)*(H9+0.3*2))*S9),IF(AND(L9=\"ดินอ่อน\",O9<=1.5),(((G9+0.2*2)*(H9+0.2*2))*S9),IF(AND(L9=\"ดินแข็ง\",O9<=1.5),(((G9+0.2*2)*(H9+0.2*2))*S9),IF(AND(L9=\"ดินแข็ง\",O9>1.5),(((G9+0.3*2)*(H9+0.3*2))*S9))))),3)","v":0},{"$f":"P9-K9+T9+R9","v":0},"RB 12 mm.","@",null,{"$f":"IF(X9=0,0,((G9/X9)+1)*(H9+(I9*2))*J9)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB9=0,0,((H9/AB9+1)*(G9+I9*2))*J9)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF9=0,0,((I9/AF9+1)*(H9*2+G9*2))*J9)","v":0},{"$f":"(G9*I9*2)+(H9*I9*2)+(D9*F9*2)+(E9*F9*2)","v":0},null,{"$f":"J9*AI9","v":0},null,"RB 12 mm.",{"$f":"IF(F9=0,0,F9+(G9/3))*AK9","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP9=0,0,(ROUNDUP(F9/AP9+1,0)*(D9*2+E9*2))*AK9)","v":0}]
[null,5,"F1-5",0.1,0.1,null,null,null,null,null,{"$f":"(D10*E10*F10+G10*H10*I10)*J10","v":0},"ดินแข็ง",{"$f":"G10","v":0},{"$f":"H10","v":0},null,{"$f":"ROUND(IF(AND(L10=\"ดินแข็ง\",O10<=1.5),((M10+0.2*2)*(N10+0.2*2))*O10,IF(AND(L10=\"ดินแข็ง\",O10>1.5),((M10+0.3*2)+(N10+0.3*2))*O10,IF(AND(O10<=1.5,L10=\"ดินอ่อน\"),1/3*O10*(((N10+0.2*2)*(M10+0.2*2))+((N10+0.3*O10*2)*(M10+0.3*O10*2))+SQRT((((N10+0.2*2)*(M10+0.2*2))*((N10+0.3*O10*2)*(M10+0.3*O10*2))))),IF(AND(O10>1.5,L10=\"ดินอ่อน\"),1/3*O10*(((N10+0.3*2)*(M10+0.3*2))+((N10+0.5*O10*2)*(M10+0.5*O10*2))+SQRT((((N10+0.3*2)*(M10+0.3*2))*((N10+0.5*O10*2)*(M10+0.5*O10*2))))))))),2)*J10","v":0},null,{"$f":"ROUND(IF(AND(L10=\"ดินอ่อน\",O10>1.5),(((G10+0.3*2)*(H10+0.3*2))*Q10),IF(AND(L10=\"ดินอ่อน\",O10<=1.5),(((G10+0.2*2)*(H10+0.2*2))*Q10),IF(AND(L10=\"ดินแข็ง\",O10<=1.5),(((G10+0.2*2)*(H10+0.2*2))*Q10),IF(AND(L10=\"ดินแข็ง\",O10>1.5),(((G10+0.3*2)*(H10+0.3*2))*Q10))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L10=\"ดินอ่อน\",O10>1.5),(((G10+0.3*2)*(H10+0.3*2))*S10),IF(AND(L10=\"ดินอ่อน\",O10<=1.5),(((G10+0.2*2)*(H10+0.2*2))*S10),IF(AND(L10=\"ดินแข็ง\",O10<=1.5),(((G10+0.2*2)*(H10+0.2*2))*S10),IF(AND(L10=\"ดินแข็ง\",O10>1.5),(((G10+0.3*2)*(H10+0.3*2))*S10))))),3)","v":0},{"$f":"P10-K10+T10+R10","v":0},"RB 12 mm.","@",null,{"$f":"IF(X10=0,0,((G10/X10)+1)*(H10+(I10*2))*J10)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB10=0,0,((H10/AB10+1)*(G10+I10*2))*J10)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF10=0,0,((I10/AF10+1)*(H10*2+G10*2))*J10)","v":0},{"$f":"(G10*I10*2)+(H10*I10*2)+(D10*F10*2)+(E10*F10*2)","v":0},null,{"$f":"J10*AI10","v":0},null,"RB 12 mm.",{"$f":"IF(F10=0,0,F10+(G10/3))*AK10","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP10=0,0,(ROUNDUP(F10/AP10+1,0)*(D10*2+E10*2))*AK10)","v":0}]
[null,6,"F1-6",0.1,0.1,null,null,null,null,null,{"$f":"(D11*E11*F11+G11*H11*I11)*J11","v":0},"ดินแข็ง",{"$f":"G11","v":0},{"$f":"H11","v":0},null,{"$f":"ROUND(IF(AND(L11=\"ดินแข็ง\",O11<=1.5),((M11+0.2*2)*(N11+0.2*2))*O11,IF(AND(L11=\"ดินแข็ง\",O11>1.5),((M11+0.3*2)+(N11+0.3*2))*O11,IF(AND(O11<=1.5,L11=\"ดินอ่อน\"),1/3*O11*(((N11+0.2*2)*(M11+0.2*2))+((N11+0.3*O11*2)*(M11+0.3*O11*2))+SQRT((((N11+0.2*2)*(M11+0.2*2))*((N11+0.3*O11*2)*(M11+0.3*O11*2))))),IF(AND(O11>1.5,L11=\"ดินอ่อน\"),1/3*O11*(((N11+0.3*2)*(M11+0.3*2))+((N11+0.5*O11*2)*(M11+0.5*O11*2))+SQRT((((N11+0.3*2)*(M11+0.3*2))*((N11+0.5*O11*2)*(M11+0.5*O11*2))))))))),2)*J11","v":0},null,{"$f":"ROUND(IF(AND(L11=\"ดินอ่อน\",O11>1.5),(((G11+0.3*2)*(H11+0.3*2))*Q11),IF(AND(L11=\"ดินอ่อน\",O11<=1.5),(((G11+0.2*2)*(H11+0.2*2))*Q11),IF(AND(L11=\"ดินแข็ง\",O11<=1.5),(((G11+0.2*2)*(H11+0.2*2))*Q11),IF(AND(L11=\"ดินแข็ง\",O11>1.5),(((G11+0.3*2)*(H11+0.3*2))*Q11))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L11=\"ดินอ่อน\",O11>1.5),(((G11+0.3*2)*(H11+0.3*2))*S11),IF(AND(L11=\"ดินอ่อน\",O11<=1.5),(((G11+0.2*2)*(H11+0.2*2))*S11),IF(AND(L11=\"ดินแข็ง\",O11<=1.5),(((G11+0.2*2)*(H11+0.2*2))*S11),IF(AND(L11=\"ดินแข็ง\",O11>1.5),(((G11+0.3*2)*(H11+0.3*2))*S11))))),3)","v":0},{"$f":"P11-K11+T11+R11","v":0},"RB 12 mm.","@",null,{"$f":"IF(X11=0,0,((G11/X11)+1)*(H11+(I11*2))*J11)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB11=0,0,((H11/AB11+1)*(G11+I11*2))*J11)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF11=0,0,((I11/AF11+1)*(H11*2+G11*2))*J11)","v":0},{"$f":"(G11*I11*2)+(H11*I11*2)+(D11*F11*2)+(E11*F11*2)","v":0},null,{"$f":"J11*AI11","v":0},null,"RB 12 mm.",{"$f":"IF(F11=0,0,F11+(G11/3))*AK11","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP11=0,0,(ROUNDUP(F11/AP11+1,0)*(D11*2+E11*2))*AK11)","v":0}]
[null,7,"F1-7",0.1,0.1,null,null,null,null,null,{"$f":"(D12*E12*F12+G12*H12*I12)*J12","v":0},"ดินแข็ง",{"$f":"G12","v":0},{"$f":"H12","v":0},null,{"$f":"ROUND(IF(AND(L12=\"ดินแข็ง\",O12<=1.5),((M12+0.2*2)*(N12+0.2*2))*O12,IF(AND(L12=\"ดินแข็ง\",O12>1.5),((M12+0.3*2)+(N12+0.3*2))*O12,IF(AND(O12<=1.5,L12=\"ดินอ่อน\"),1/3*O12*(((N12+0.2*2)*(M12+0.2*2))+((N12+0.3*O12*2)*(M12+0.3*O12*2))+SQRT((((N12+0.2*2)*(M12+0.2*2))*((N12+0.3*O12*2)*(M12+0.3*O12*2))))),IF(AND(O12>1.5,L12=\"ดินอ่อน\"),1/3*O12*(((N12+0.3*2)*(M12+0.3*2))+((N12+0.5*O12*2)*(M12+0.5*O12*2))+SQRT((((N12+0.3*2)*(M12+0.3*2))*((N12+0.5*O12*2)*(M12+0.5*O12*2))))))))),2)*J12","v":0},null,{"$f":"ROUND(IF(AND(L12=\"ดินอ่อน\",O12>1.5),(((G12+0.3*2)*(H12+0.3*2))*Q12),IF(AND(L12=\"ดินอ่อน\",O12<=1.5),(((G12+0.2*2)*(H12+0.2*2))*Q12),IF(AND(L12=\"ดินแข็ง\",O12<=1.5),(((G12+0.2*2)*(H12+0.2*2))*Q12),IF(AND(L12=\"ดินแข็ง\",O12>1.5),(((G12+0.3*2)*(H12+0.3*2))*Q12))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L12=\"ดินอ่อน\",O12>1.5),(((G12+0.3*2)*(H12+0.3*2))*S12),IF(AND(L12=\"ดินอ่อน\",O12<=1.5),(((G12+0.2*2)*(H12+0.2*2))*S12),IF(AND(L12=\"ดินแข็ง\",O12<=1.5),(((G12+0.2*2)*(H12+0.2*2))*S12),IF(AND(L12=\"ดินแข็ง\",O12>1.5),(((G12+0.3*2)*(H12+0.3*2))*S12))))),3)","v":0},{"$f":"P12-K12+T12+R12","v":0},"RB 12 mm.","@",null,{"$f":"IF(X12=0,0,((G12/X12)+1)*(H12+(I12*2))*J12)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB12=0,0,((H12/AB12+1)*(G12+I12*2))*J12)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF12=0,0,((I12/AF12+1)*(H12*2+G12*2))*J12)","v":0},{"$f":"(G12*I12*2)+(H12*I12*2)+(D12*F12*2)+(E12*F12*2)","v":0},null,{"$f":"J12*AI12","v":0},null,"RB 12 mm.",{"$f":"IF(F12=0,0,F12+(G12/3))*AK12","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP12=0,0,(ROUNDUP(F12/AP12+1,0)*(D12*2+E12*2))*AK12)","v":0}]
[null,8,"F1-8",0.1,0.1,null,null,null,null,null,{"$f":"(D13*E13*F13+G13*H13*I13)*J13","v":0},"ดินแข็ง",{"$f":"G13","v":0},{"$f":"H13","v":0},null,{"$f":"ROUND(IF(AND(L13=\"ดินแข็ง\",O13<=1.5),((M13+0.2*2)*(N13+0.2*2))*O13,IF(AND(L13=\"ดินแข็ง\",O13>1.5),((M13+0.3*2)+(N13+0.3*2))*O13,IF(AND(O13<=1.5,L13=\"ดินอ่อน\"),1/3*O13*(((N13+0.2*2)*(M13+0.2*2))+((N13+0.3*O13*2)*(M13+0.3*O13*2))+SQRT((((N13+0.2*2)*(M13+0.2*2))*((N13+0.3*O13*2)*(M13+0.3*O13*2))))),IF(AND(O13>1.5,L13=\"ดินอ่อน\"),1/3*O13*(((N13+0.3*2)*(M13+0.3*2))+((N13+0.5*O13*2)*(M13+0.5*O13*2))+SQRT((((N13+0.3*2)*(M13+0.3*2))*((N13+0.5*O13*2)*(M13+0.5*O13*2))))))))),2)*J13","v":0},null,{"$f":"ROUND(IF(AND(L13=\"ดินอ่อน\",O13>1.5),(((G13+0.3*2)*(H13+0.3*2))*Q13),IF(AND(L13=\"ดินอ่อน\",O13<=1.5),(((G13+0.2*2)*(H13+0.2*2))*Q13),IF(AND(L13=\"ดินแข็ง\",O13<=1.5),(((G13+0.2*2)*(H13+0.2*2))*Q13),IF(AND(L13=\"ดินแข็ง\",O13>1.5),(((G13+0.3*2)*(H13+0.3*2))*Q13))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L13=\"ดินอ่อน\",O13>1.5),(((G13+0.3*2)*(H13+0.3*2))*S13),IF(AND(L13=\"ดินอ่อน\",O13<=1.5),(((G13+0.2*2)*(H13+0.2*2))*S13),IF(AND(L13=\"ดินแข็ง\",O13<=1.5),(((G13+0.2*2)*(H13+0.2*2))*S13),IF(AND(L13=\"ดินแข็ง\",O13>1.5),(((G13+0.3*2)*(H13+0.3*2))*S13))))),3)","v":0},{"$f":"P13-K13+T13+R13","v":0},"RB 12 mm.","@",null,{"$f":"IF(X13=0,0,((G13/X13)+1)*(H13+(I13*2))*J13)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB13=0,0,((H13/AB13+1)*(G13+I13*2))*J13)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF13=0,0,((I13/AF13+1)*(H13*2+G13*2))*J13)","v":0},{"$f":"(G13*I13*2)+(H13*I13*2)+(D13*F13*2)+(E13*F13*2)","v":0},null,{"$f":"J13*AI13","v":0},null,"RB 12 mm.",{"$f":"IF(F13=0,0,F13+(G13/3))*AK13","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP13=0,0,(ROUNDUP(F13/AP13+1,0)*(D13*2+E13*2))*AK13)","v":0}]
[null,9,"F1-9",0.1,0.1,null,null,null,null,null,{"$f":"(D14*E14*F14+G14*H14*I14)*J14","v":0},"ดินแข็ง",{"$f":"G14","v":0},{"$f":"H14","v":0},null,{"$f":"ROUND(IF(AND(L14=\"ดินแข็ง\",O14<=1.5),((M14+0.2*2)*(N14+0.2*2))*O14,IF(AND(L14=\"ดินแข็ง\",O14>1.5),((M14+0.3*2)+(N14+0.3*2))*O14,IF(AND(O14<=1.5,L14=\"ดินอ่อน\"),1/3*O14*(((N14+0.2*2)*(M14+0.2*2))+((N14+0.3*O14*2)*(M14+0.3*O14*2))+SQRT((((N14+0.2*2)*(M14+0.2*2))*((N14+0.3*O14*2)*(M14+0.3*O14*2))))),IF(AND(O14>1.5,L14=\"ดินอ่อน\"),1/3*O14*(((N14+0.3*2)*(M14+0.3*2))+((N14+0.5*O14*2)*(M14+0.5*O14*2))+SQRT((((N14+0.3*2)*(M14+0.3*2))*((N14+0.5*O14*2)*(M14+0.5*O14*2))))))))),2)*J14","v":0},null,{"$f":"ROUND(IF(AND(L14=\"ดินอ่อน\",O14>1.5),(((G14+0.3*2)*(H14+0.3*2))*Q14),IF(AND(L14=\"ดินอ่อน\",O14<=1.5),(((G14+0.2*2)*(H14+0.2*2))*Q14),IF(AND(L14=\"ดินแข็ง\",O14<=1.5),(((G14+0.2*2)*(H14+0.2*2))*Q14),IF(AND(L14=\"ดินแข็ง\",O14>1.5),(((G14+0.3*2)*(H14+0.3*2))*Q14))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L14=\"ดินอ่อน\",O14>1.5),(((G14+0.3*2)*(H14+0.3*2))*S14),IF(AND(L14=\"ดินอ่อน\",O14<=1.5),(((G14+0.2*2)*(H14+0.2*2))*S14),IF(AND(L14=\"ดินแข็ง\",O14<=1.5),(((G14+0.2*2)*(H14+0.2*2))*S14),IF(AND(L14=\"ดินแข็ง\",O14>1.5),(((G14+0.3*2)*(H14+0.3*2))*S14))))),3)","v":0},{"$f":"P14-K14+T14+R14","v":0},"RB 12 mm.","@",null,{"$f":"IF(X14=0,0,((G14/X14)+1)*(H14+(I14*2))*J14)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB14=0,0,((H14/AB14+1)*(G14+I14*2))*J14)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF14=0,0,((I14/AF14+1)*(H14*2+G14*2))*J14)","v":0},{"$f":"(G14*I14*2)+(H14*I14*2)+(D14*F14*2)+(E14*F14*2)","v":0},null,{"$f":"J14*AI14","v":0},null,"RB 12 mm.",{"$f":"IF(F14=0,0,F14+(G14/3))*AK14","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP14=0,0,(ROUNDUP(F14/AP14+1,0)*(D14*2+E14*2))*AK14)","v":0}]
[null,10,"F1-10",0.1,0.1,null,null,null,null,null,{"$f":"(D15*E15*F15+G15*H15*I15)*J15","v":0},"ดินแข็ง",{"$f":"G15","v":0},{"$f":"H15","v":0},null,{"$f":"ROUND(IF(AND(L15=\"ดินแข็ง\",O15<=1.5),((M15+0.2*2)*(N15+0.2*2))*O15,IF(AND(L15=\"ดินแข็ง\",O15>1.5),((M15+0.3*2)+(N15+0.3*2))*O15,IF(AND(O15<=1.5,L15=\"ดินอ่อน\"),1/3*O15*(((N15+0.2*2)*(M15+0.2*2))+((N15+0.3*O15*2)*(M15+0.3*O15*2))+SQRT((((N15+0.2*2)*(M15+0.2*2))*((N15+0.3*O15*2)*(M15+0.3*O15*2))))),IF(AND(O15>1.5,L15=\"ดินอ่อน\"),1/3*O15*(((N15+0.3*2)*(M15+0.3*2))+((N15+0.5*O15*2)*(M15+0.5*O15*2))+SQRT((((N15+0.3*2)*(M15+0.3*2))*((N15+0.5*O15*2)*(M15+0.5*O15*2))))))))),2)*J15","v":0},null,{"$f":"ROUND(IF(AND(L15=\"ดินอ่อน\",O15>1.5),(((G15+0.3*2)*(H15+0.3*2))*Q15),IF(AND(L15=\"ดินอ่อน\",O15<=1.5),(((G15+0.2*2)*(H15+0.2*2))*Q15),IF(AND(L15=\"ดินแข็ง\",O15<=1.5),(((G15+0.2*2)*(H15+0.2*2))*Q15),IF(AND(L15=\"ดินแข็ง\",O15>1.5),(((G15+0.3*2)*(H15+0.3*2))*Q15))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L15=\"ดินอ่อน\",O15>1.5),(((G15+0.3*2)*(H15+0.3*2))*S15),IF(AND(L15=\"ดินอ่อน\",O15<=1.5),(((G15+0.2*2)*(H15+0.2*2))*S15),IF(AND(L15=\"ดินแข็ง\",O15<=1.5),(((G15+0.2*2)*(H15+0.2*2))*S15),IF(AND(L15=\"ดินแข็ง\",O15>1.5),(((G15+0.3*2)*(H15+0.3*2))*S15))))),3)","v":0},{"$f":"P15-K15+T15+R15","v":0},"RB 12 mm.","@",null,{"$f":"IF(X15=0,0,((G15/X15)+1)*(H15+(I15*2))*J15)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB15=0,0,((H15/AB15+1)*(G15+I15*2))*J15)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF15=0,0,((I15/AF15+1)*(H15*2+G15*2))*J15)","v":0},{"$f":"(G15*I15*2)+(H15*I15*2)+(D15*F15*2)+(E15*F15*2)","v":0},null,{"$f":"J15*AI15","v":0},null,"RB 12 mm.",{"$f":"IF(F15=0,0,F15+(G15/3))*AK15","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP15=0,0,(ROUNDUP(F15/AP15+1,0)*(D15*2+E15*2))*AK15)","v":0}]
[null,11,"F1-11",0.1,0.1,null,null,null,null,null,{"$f":"(D16*E16*F16+G16*H16*I16)*J16","v":0},"ดินแข็ง",{"$f":"G16","v":0},{"$f":"H16","v":0},null,{"$f":"ROUND(IF(AND(L16=\"ดินแข็ง\",O16<=1.5),((M16+0.2*2)*(N16+0.2*2))*O16,IF(AND(L16=\"ดินแข็ง\",O16>1.5),((M16+0.3*2)+(N16+0.3*2))*O16,IF(AND(O16<=1.5,L16=\"ดินอ่อน\"),1/3*O16*(((N16+0.2*2)*(M16+0.2*2))+((N16+0.3*O16*2)*(M16+0.3*O16*2))+SQRT((((N16+0.2*2)*(M16+0.2*2))*((N16+0.3*O16*2)*(M16+0.3*O16*2))))),IF(AND(O16>1.5,L16=\"ดินอ่อน\"),1/3*O16*(((N16+0.3*2)*(M16+0.3*2))+((N16+0.5*O16*2)*(M16+0.5*O16*2))+SQRT((((N16+0.3*2)*(M16+0.3*2))*((N16+0.5*O16*2)*(M16+0.5*O16*2))))))))),2)*J16","v":0},null,{"$f":"ROUND(IF(AND(L16=\"ดินอ่อน\",O16>1.5),(((G16+0.3*2)*(H16+0.3*2))*Q16),IF(AND(L16=\"ดินอ่อน\",O16<=1.5),(((G16+0.2*2)*(H16+0.2*2))*Q16),IF(AND(L16=\"ดินแข็ง\",O16<=1.5),(((G16+0.2*2)*(H16+0.2*2))*Q16),IF(AND(L16=\"ดินแข็ง\",O16>1.5),(((G16+0.3*2)*(H16+0.3*2))*Q16))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L16=\"ดินอ่อน\",O16>1.5),(((G16+0.3*2)*(H16+0.3*2))*S16),IF(AND(L16=\"ดินอ่อน\",O16<=1.5),(((G16+0.2*2)*(H16+0.2*2))*S16),IF(AND(L16=\"ดินแข็ง\",O16<=1.5),(((G16+0.2*2)*(H16+0.2*2))*S16),IF(AND(L16=\"ดินแข็ง\",O16>1.5),(((G16+0.3*2)*(H16+0.3*2))*S16))))),3)","v":0},{"$f":"P16-K16+T16+R16","v":0},"RB 12 mm.","@",null,{"$f":"IF(X16=0,0,((G16/X16)+1)*(H16+(I16*2))*J16)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB16=0,0,((H16/AB16+1)*(G16+I16*2))*J16)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF16=0,0,((I16/AF16+1)*(H16*2+G16*2))*J16)","v":0},{"$f":"(G16*I16*2)+(H16*I16*2)+(D16*F16*2)+(E16*F16*2)","v":0},null,{"$f":"J16*AI16","v":0},null,"RB 12 mm.",{"$f":"IF(F16=0,0,F16+(G16/3))*AK16","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP16=0,0,(ROUNDUP(F16/AP16+1,0)*(D16*2+E16*2))*AK16)","v":0}]
[null,12,"F1-12",0.1,0.1,null,null,null,null,null,{"$f":"(D17*E17*F17+G17*H17*I17)*J17","v":0},"ดินแข็ง",{"$f":"G17","v":0},{"$f":"H17","v":0},null,{"$f":"ROUND(IF(AND(L17=\"ดินแข็ง\",O17<=1.5),((M17+0.2*2)*(N17+0.2*2))*O17,IF(AND(L17=\"ดินแข็ง\",O17>1.5),((M17+0.3*2)+(N17+0.3*2))*O17,IF(AND(O17<=1.5,L17=\"ดินอ่อน\"),1/3*O17*(((N17+0.2*2)*(M17+0.2*2))+((N17+0.3*O17*2)*(M17+0.3*O17*2))+SQRT((((N17+0.2*2)*(M17+0.2*2))*((N17+0.3*O17*2)*(M17+0.3*O17*2))))),IF(AND(O17>1.5,L17=\"ดินอ่อน\"),1/3*O17*(((N17+0.3*2)*(M17+0.3*2))+((N17+0.5*O17*2)*(M17+0.5*O17*2))+SQRT((((N17+0.3*2)*(M17+0.3*2))*((N17+0.5*O17*2)*(M17+0.5*O17*2))))))))),2)*J17","v":0},null,{"$f":"ROUND(IF(AND(L17=\"ดินอ่อน\",O17>1.5),(((G17+0.3*2)*(H17+0.3*2))*Q17),IF(AND(L17=\"ดินอ่อน\",O17<=1.5),(((G17+0.2*2)*(H17+0.2*2))*Q17),IF(AND(L17=\"ดินแข็ง\",O17<=1.5),(((G17+0.2*2)*(H17+0.2*2))*Q17),IF(AND(L17=\"ดินแข็ง\",O17>1.5),(((G17+0.3*2)*(H17+0.3*2))*Q17))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L17=\"ดินอ่อน\",O17>1.5),(((G17+0.3*2)*(H17+0.3*2))*S17),IF(AND(L17=\"ดินอ่อน\",O17<=1.5),(((G17+0.2*2)*(H17+0.2*2))*S17),IF(AND(L17=\"ดินแข็ง\",O17<=1.5),(((G17+0.2*2)*(H17+0.2*2))*S17),IF(AND(L17=\"ดินแข็ง\",O17>1.5),(((G17+0.3*2)*(H17+0.3*2))*S17))))),3)","v":0},{"$f":"P17-K17+T17+R17","v":0},"RB 12 mm.","@",null,{"$f":"IF(X17=0,0,((G17/X17)+1)*(H17+(I17*2))*J17)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB17=0,0,((H17/AB17+1)*(G17+I17*2))*J17)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF17=0,0,((I17/AF17+1)*(H17*2+G17*2))*J17)","v":0},{"$f":"(G17*I17*2)+(H17*I17*2)+(D17*F17*2)+(E17*F17*2)","v":0},null,{"$f":"J17*AI17","v":0},null,"RB 12 mm.",{"$f":"IF(F17=0,0,F17+(G17/3))*AK17","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP17=0,0,(ROUNDUP(F17/AP17+1,0)*(D17*2+E17*2))*AK17)","v":0}]
[null,13,"F1-13",0.1,0.1,null,null,null,null,null,{"$f":"(D18*E18*F18+G18*H18*I18)*J18","v":0},"ดินแข็ง",{"$f":"G18","v":0},{"$f":"H18","v":0},null,{"$f":"ROUND(IF(AND(L18=\"ดินแข็ง\",O18<=1.5),((M18+0.2*2)*(N18+0.2*2))*O18,IF(AND(L18=\"ดินแข็ง\",O18>1.5),((M18+0.3*2)+(N18+0.3*2))*O18,IF(AND(O18<=1.5,L18=\"ดินอ่อน\"),1/3*O18*(((N18+0.2*2)*(M18+0.2*2))+((N18+0.3*O18*2)*(M18+0.3*O18*2))+SQRT((((N18+0.2*2)*(M18+0.2*2))*((N18+0.3*O18*2)*(M18+0.3*O18*2))))),IF(AND(O18>1.5,L18=\"ดินอ่อน\"),1/3*O18*(((N18+0.3*2)*(M18+0.3*2))+((N18+0.5*O18*2)*(M18+0.5*O18*2))+SQRT((((N18+0.3*2)*(M18+0.3*2))*((N18+0.5*O18*2)*(M18+0.5*O18*2))))))))),2)*J18","v":0},null,{"$f":"ROUND(IF(AND(L18=\"ดินอ่อน\",O18>1.5),(((G18+0.3*2)*(H18+0.3*2))*Q18),IF(AND(L18=\"ดินอ่อน\",O18<=1.5),(((G18+0.2*2)*(H18+0.2*2))*Q18),IF(AND(L18=\"ดินแข็ง\",O18<=1.5),(((G18+0.2*2)*(H18+0.2*2))*Q18),IF(AND(L18=\"ดินแข็ง\",O18>1.5),(((G18+0.3*2)*(H18+0.3*2))*Q18))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L18=\"ดินอ่อน\",O18>1.5),(((G18+0.3*2)*(H18+0.3*2))*S18),IF(AND(L18=\"ดินอ่อน\",O18<=1.5),(((G18+0.2*2)*(H18+0.2*2))*S18),IF(AND(L18=\"ดินแข็ง\",O18<=1.5),(((G18+0.2*2)*(H18+0.2*2))*S18),IF(AND(L18=\"ดินแข็ง\",O18>1.5),(((G18+0.3*2)*(H18+0.3*2))*S18))))),3)","v":0},{"$f":"P18-K18+T18+R18","v":0},"RB 12 mm.","@",null,{"$f":"IF(X18=0,0,((G18/X18)+1)*(H18+(I18*2))*J18)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB18=0,0,((H18/AB18+1)*(G18+I18*2))*J18)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF18=0,0,((I18/AF18+1)*(H18*2+G18*2))*J18)","v":0},{"$f":"(G18*I18*2)+(H18*I18*2)+(D18*F18*2)+(E18*F18*2)","v":0},null,{"$f":"J18*AI18","v":0},null,"RB 12 mm.",{"$f":"IF(F18=0,0,F18+(G18/3))*AK18","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP18=0,0,(ROUNDUP(F18/AP18+1,0)*(D18*2+E18*2))*AK18)","v":0}]
[null,14,"F1-14",0.1,0.1,null,null,null,null,null,{"$f":"(D19*E19*F19+G19*H19*I19)*J19","v":0},"ดินแข็ง",{"$f":"G19","v":0},{"$f":"H19","v":0},null,{"$f":"ROUND(IF(AND(L19=\"ดินแข็ง\",O19<=1.5),((M19+0.2*2)*(N19+0.2*2))*O19,IF(AND(L19=\"ดินแข็ง\",O19>1.5),((M19+0.3*2)+(N19+0.3*2))*O19,IF(AND(O19<=1.5,L19=\"ดินอ่อน\"),1/3*O19*(((N19+0.2*2)*(M19+0.2*2))+((N19+0.3*O19*2)*(M19+0.3*O19*2))+SQRT((((N19+0.2*2)*(M19+0.2*2))*((N19+0.3*O19*2)*(M19+0.3*O19*2))))),IF(AND(O19>1.5,L19=\"ดินอ่อน\"),1/3*O19*(((N19+0.3*2)*(M19+0.3*2))+((N19+0.5*O19*2)*(M19+0.5*O19*2))+SQRT((((N19+0.3*2)*(M19+0.3*2))*((N19+0.5*O19*2)*(M19+0.5*O19*2))))))))),2)*J19","v":0},null,{"$f":"ROUND(IF(AND(L19=\"ดินอ่อน\",O19>1.5),(((G19+0.3*2)*(H19+0.3*2))*Q19),IF(AND(L19=\"ดินอ่อน\",O19<=1.5),(((G19+0.2*2)*(H19+0.2*2))*Q19),IF(AND(L19=\"ดินแข็ง\",O19<=1.5),(((G19+0.2*2)*(H19+0.2*2))*Q19),IF(AND(L19=\"ดินแข็ง\",O19>1.5),(((G19+0.3*2)*(H19+0.3*2))*Q19))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L19=\"ดินอ่อน\",O19>1.5),(((G19+0.3*2)*(H19+0.3*2))*S19),IF(AND(L19=\"ดินอ่อน\",O19<=1.5),(((G19+0.2*2)*(H19+0.2*2))*S19),IF(AND(L19=\"ดินแข็ง\",O19<=1.5),(((G19+0.2*2)*(H19+0.2*2))*S19),IF(AND(L19=\"ดินแข็ง\",O19>1.5),(((G19+0.3*2)*(H19+0.3*2))*S19))))),3)","v":0},{"$f":"P19-K19+T19+R19","v":0},"RB 12 mm.","@",null,{"$f":"IF(X19=0,0,((G19/X19)+1)*(H19+(I19*2))*J19)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB19=0,0,((H19/AB19+1)*(G19+I19*2))*J19)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF19=0,0,((I19/AF19+1)*(H19*2+G19*2))*J19)","v":0},{"$f":"(G19*I19*2)+(H19*I19*2)+(D19*F19*2)+(E19*F19*2)","v":0},null,{"$f":"J19*AI19","v":0},null,"RB 12 mm.",{"$f":"IF(F19=0,0,F19+(G19/3))*AK19","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP19=0,0,(ROUNDUP(F19/AP19+1,0)*(D19*2+E19*2))*AK19)","v":0}]
[null,15,"F1-15",0.1,0.1,null,null,null,null,null,{"$f":"(D20*E20*F20+G20*H20*I20)*J20","v":0},"ดินแข็ง",{"$f":"G20","v":0},{"$f":"H20","v":0},null,{"$f":"ROUND(IF(AND(L20=\"ดินแข็ง\",O20<=1.5),((M20+0.2*2)*(N20+0.2*2))*O20,IF(AND(L20=\"ดินแข็ง\",O20>1.5),((M20+0.3*2)+(N20+0.3*2))*O20,IF(AND(O20<=1.5,L20=\"ดินอ่อน\"),1/3*O20*(((N20+0.2*2)*(M20+0.2*2))+((N20+0.3*O20*2)*(M20+0.3*O20*2))+SQRT((((N20+0.2*2)*(M20+0.2*2))*((N20+0.3*O20*2)*(M20+0.3*O20*2))))),IF(AND(O20>1.5,L20=\"ดินอ่อน\"),1/3*O20*(((N20+0.3*2)*(M20+0.3*2))+((N20+0.5*O20*2)*(M20+0.5*O20*2))+SQRT((((N20+0.3*2)*(M20+0.3*2))*((N20+0.5*O20*2)*(M20+0.5*O20*2))))))))),2)*J20","v":0},null,{"$f":"ROUND(IF(AND(L20=\"ดินอ่อน\",O20>1.5),(((G20+0.3*2)*(H20+0.3*2))*Q20),IF(AND(L20=\"ดินอ่อน\",O20<=1.5),(((G20+0.2*2)*(H20+0.2*2))*Q20),IF(AND(L20=\"ดินแข็ง\",O20<=1.5),(((G20+0.2*2)*(H20+0.2*2))*Q20),IF(AND(L20=\"ดินแข็ง\",O20>1.5),(((G20+0.3*2)*(H20+0.3*2))*Q20))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L20=\"ดินอ่อน\",O20>1.5),(((G20+0.3*2)*(H20+0.3*2))*S20),IF(AND(L20=\"ดินอ่อน\",O20<=1.5),(((G20+0.2*2)*(H20+0.2*2))*S20),IF(AND(L20=\"ดินแข็ง\",O20<=1.5),(((G20+0.2*2)*(H20+0.2*2))*S20),IF(AND(L20=\"ดินแข็ง\",O20>1.5),(((G20+0.3*2)*(H20+0.3*2))*S20))))),3)","v":0},{"$f":"P20-K20+T20+R20","v":0},"RB 12 mm.","@",null,{"$f":"IF(X20=0,0,((G20/X20)+1)*(H20+(I20*2))*J20)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB20=0,0,((H20/AB20+1)*(G20+I20*2))*J20)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF20=0,0,((I20/AF20+1)*(H20*2+G20*2))*J20)","v":0},{"$f":"(G20*I20*2)+(H20*I20*2)+(D20*F20*2)+(E20*F20*2)","v":0},null,{"$f":"J20*AI20","v":0},null,"RB 12 mm.",{"$f":"IF(F20=0,0,F20+(G20/3))*AK20","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP20=0,0,(ROUNDUP(F20/AP20+1,0)*(D20*2+E20*2))*AK20)","v":0}]
[null,16,"F1-16",0.1,0.1,null,null,null,null,null,{"$f":"(D21*E21*F21+G21*H21*I21)*J21","v":0},"ดินแข็ง",{"$f":"G21","v":0},{"$f":"H21","v":0},null,{"$f":"ROUND(IF(AND(L21=\"ดินแข็ง\",O21<=1.5),((M21+0.2*2)*(N21+0.2*2))*O21,IF(AND(L21=\"ดินแข็ง\",O21>1.5),((M21+0.3*2)+(N21+0.3*2))*O21,IF(AND(O21<=1.5,L21=\"ดินอ่อน\"),1/3*O21*(((N21+0.2*2)*(M21+0.2*2))+((N21+0.3*O21*2)*(M21+0.3*O21*2))+SQRT((((N21+0.2*2)*(M21+0.2*2))*((N21+0.3*O21*2)*(M21+0.3*O21*2))))),IF(AND(O21>1.5,L21=\"ดินอ่อน\"),1/3*O21*(((N21+0.3*2)*(M21+0.3*2))+((N21+0.5*O21*2)*(M21+0.5*O21*2))+SQRT((((N21+0.3*2)*(M21+0.3*2))*((N21+0.5*O21*2)*(M21+0.5*O21*2))))))))),2)*J21","v":0},null,{"$f":"ROUND(IF(AND(L21=\"ดินอ่อน\",O21>1.5),(((G21+0.3*2)*(H21+0.3*2))*Q21),IF(AND(L21=\"ดินอ่อน\",O21<=1.5),(((G21+0.2*2)*(H21+0.2*2))*Q21),IF(AND(L21=\"ดินแข็ง\",O21<=1.5),(((G21+0.2*2)*(H21+0.2*2))*Q21),IF(AND(L21=\"ดินแข็ง\",O21>1.5),(((G21+0.3*2)*(H21+0.3*2))*Q21))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L21=\"ดินอ่อน\",O21>1.5),(((G21+0.3*2)*(H21+0.3*2))*S21),IF(AND(L21=\"ดินอ่อน\",O21<=1.5),(((G21+0.2*2)*(H21+0.2*2))*S21),IF(AND(L21=\"ดินแข็ง\",O21<=1.5),(((G21+0.2*2)*(H21+0.2*2))*S21),IF(AND(L21=\"ดินแข็ง\",O21>1.5),(((G21+0.3*2)*(H21+0.3*2))*S21))))),3)","v":0},{"$f":"P21-K21+T21+R21","v":0},"RB 12 mm.","@",null,{"$f":"IF(X21=0,0,((G21/X21)+1)*(H21+(I21*2))*J21)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB21=0,0,((H21/AB21+1)*(G21+I21*2))*J21)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF21=0,0,((I21/AF21+1)*(H21*2+G21*2))*J21)","v":0},{"$f":"(G21*I21*2)+(H21*I21*2)+(D21*F21*2)+(E21*F21*2)","v":0},null,{"$f":"J21*AI21","v":0},null,"RB 12 mm.",{"$f":"IF(F21=0,0,F21+(G21/3))*AK21","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP21=0,0,(ROUNDUP(F21/AP21+1,0)*(D21*2+E21*2))*AK21)","v":0}]
[null,17,"F1-17",0.1,0.1,null,null,null,null,null,{"$f":"(D22*E22*F22+G22*H22*I22)*J22","v":0},"ดินแข็ง",{"$f":"G22","v":0},{"$f":"H22","v":0},null,{"$f":"ROUND(IF(AND(L22=\"ดินแข็ง\",O22<=1.5),((M22+0.2*2)*(N22+0.2*2))*O22,IF(AND(L22=\"ดินแข็ง\",O22>1.5),((M22+0.3*2)+(N22+0.3*2))*O22,IF(AND(O22<=1.5,L22=\"ดินอ่อน\"),1/3*O22*(((N22+0.2*2)*(M22+0.2*2))+((N22+0.3*O22*2)*(M22+0.3*O22*2))+SQRT((((N22+0.2*2)*(M22+0.2*2))*((N22+0.3*O22*2)*(M22+0.3*O22*2))))),IF(AND(O22>1.5,L22=\"ดินอ่อน\"),1/3*O22*(((N22+0.3*2)*(M22+0.3*2))+((N22+0.5*O22*2)*(M22+0.5*O22*2))+SQRT((((N22+0.3*2)*(M22+0.3*2))*((N22+0.5*O22*2)*(M22+0.5*O22*2))))))))),2)*J22","v":0},null,{"$f":"ROUND(IF(AND(L22=\"ดินอ่อน\",O22>1.5),(((G22+0.3*2)*(H22+0.3*2))*Q22),IF(AND(L22=\"ดินอ่อน\",O22<=1.5),(((G22+0.2*2)*(H22+0.2*2))*Q22),IF(AND(L22=\"ดินแข็ง\",O22<=1.5),(((G22+0.2*2)*(H22+0.2*2))*Q22),IF(AND(L22=\"ดินแข็ง\",O22>1.5),(((G22+0.3*2)*(H22+0.3*2))*Q22))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L22=\"ดินอ่อน\",O22>1.5),(((G22+0.3*2)*(H22+0.3*2))*S22),IF(AND(L22=\"ดินอ่อน\",O22<=1.5),(((G22+0.2*2)*(H22+0.2*2))*S22),IF(AND(L22=\"ดินแข็ง\",O22<=1.5),(((G22+0.2*2)*(H22+0.2*2))*S22),IF(AND(L22=\"ดินแข็ง\",O22>1.5),(((G22+0.3*2)*(H22+0.3*2))*S22))))),3)","v":0},{"$f":"P22-K22+T22+R22","v":0},"RB 12 mm.","@",null,{"$f":"IF(X22=0,0,((G22/X22)+1)*(H22+(I22*2))*J22)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB22=0,0,((H22/AB22+1)*(G22+I22*2))*J22)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF22=0,0,((I22/AF22+1)*(H22*2+G22*2))*J22)","v":0},{"$f":"(G22*I22*2)+(H22*I22*2)+(D22*F22*2)+(E22*F22*2)","v":0},null,{"$f":"J22*AI22","v":0},null,"RB 12 mm.",{"$f":"IF(F22=0,0,F22+(G22/3))*AK22","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP22=0,0,(ROUNDUP(F22/AP22+1,0)*(D22*2+E22*2))*AK22)","v":0}]
[null,18,"F1-18",0.1,0.1,null,null,null,null,null,{"$f":"(D23*E23*F23+G23*H23*I23)*J23","v":0},"ดินแข็ง",{"$f":"G23","v":0},{"$f":"H23","v":0},null,{"$f":"ROUND(IF(AND(L23=\"ดินแข็ง\",O23<=1.5),((M23+0.2*2)*(N23+0.2*2))*O23,IF(AND(L23=\"ดินแข็ง\",O23>1.5),((M23+0.3*2)+(N23+0.3*2))*O23,IF(AND(O23<=1.5,L23=\"ดินอ่อน\"),1/3*O23*(((N23+0.2*2)*(M23+0.2*2))+((N23+0.3*O23*2)*(M23+0.3*O23*2))+SQRT((((N23+0.2*2)*(M23+0.2*2))*((N23+0.3*O23*2)*(M23+0.3*O23*2))))),IF(AND(O23>1.5,L23=\"ดินอ่อน\"),1/3*O23*(((N23+0.3*2)*(M23+0.3*2))+((N23+0.5*O23*2)*(M23+0.5*O23*2))+SQRT((((N23+0.3*2)*(M23+0.3*2))*((N23+0.5*O23*2)*(M23+0.5*O23*2))))))))),2)*J23","v":0},null,{"$f":"ROUND(IF(AND(L23=\"ดินอ่อน\",O23>1.5),(((G23+0.3*2)*(H23+0.3*2))*Q23),IF(AND(L23=\"ดินอ่อน\",O23<=1.5),(((G23+0.2*2)*(H23+0.2*2))*Q23),IF(AND(L23=\"ดินแข็ง\",O23<=1.5),(((G23+0.2*2)*(H23+0.2*2))*Q23),IF(AND(L23=\"ดินแข็ง\",O23>1.5),(((G23+0.3*2)*(H23+0.3*2))*Q23))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L23=\"ดินอ่อน\",O23>1.5),(((G23+0.3*2)*(H23+0.3*2))*S23),IF(AND(L23=\"ดินอ่อน\",O23<=1.5),(((G23+0.2*2)*(H23+0.2*2))*S23),IF(AND(L23=\"ดินแข็ง\",O23<=1.5),(((G23+0.2*2)*(H23+0.2*2))*S23),IF(AND(L23=\"ดินแข็ง\",O23>1.5),(((G23+0.3*2)*(H23+0.3*2))*S23))))),3)","v":0},{"$f":"P23-K23+T23+R23","v":0},"RB 12 mm.","@",null,{"$f":"IF(X23=0,0,((G23/X23)+1)*(H23+(I23*2))*J23)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB23=0,0,((H23/AB23+1)*(G23+I23*2))*J23)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF23=0,0,((I23/AF23+1)*(H23*2+G23*2))*J23)","v":0},{"$f":"(G23*I23*2)+(H23*I23*2)+(D23*F23*2)+(E23*F23*2)","v":0},null,{"$f":"J23*AI23","v":0},null,"RB 12 mm.",{"$f":"IF(F23=0,0,F23+(G23/3))*AK23","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP23=0,0,(ROUNDUP(F23/AP23+1,0)*(D23*2+E23*2))*AK23)","v":0}]
[null,19,"F1-19",0.1,0.1,null,null,null,null,null,{"$f":"(D24*E24*F24+G24*H24*I24)*J24","v":0},"ดินแข็ง",{"$f":"G24","v":0},{"$f":"H24","v":0},null,{"$f":"ROUND(IF(AND(L24=\"ดินแข็ง\",O24<=1.5),((M24+0.2*2)*(N24+0.2*2))*O24,IF(AND(L24=\"ดินแข็ง\",O24>1.5),((M24+0.3*2)+(N24+0.3*2))*O24,IF(AND(O24<=1.5,L24=\"ดินอ่อน\"),1/3*O24*(((N24+0.2*2)*(M24+0.2*2))+((N24+0.3*O24*2)*(M24+0.3*O24*2))+SQRT((((N24+0.2*2)*(M24+0.2*2))*((N24+0.3*O24*2)*(M24+0.3*O24*2))))),IF(AND(O24>1.5,L24=\"ดินอ่อน\"),1/3*O24*(((N24+0.3*2)*(M24+0.3*2))+((N24+0.5*O24*2)*(M24+0.5*O24*2))+SQRT((((N24+0.3*2)*(M24+0.3*2))*((N24+0.5*O24*2)*(M24+0.5*O24*2))))))))),2)*J24","v":0},null,{"$f":"ROUND(IF(AND(L24=\"ดินอ่อน\",O24>1.5),(((G24+0.3*2)*(H24+0.3*2))*Q24),IF(AND(L24=\"ดินอ่อน\",O24<=1.5),(((G24+0.2*2)*(H24+0.2*2))*Q24),IF(AND(L24=\"ดินแข็ง\",O24<=1.5),(((G24+0.2*2)*(H24+0.2*2))*Q24),IF(AND(L24=\"ดินแข็ง\",O24>1.5),(((G24+0.3*2)*(H24+0.3*2))*Q24))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L24=\"ดินอ่อน\",O24>1.5),(((G24+0.3*2)*(H24+0.3*2))*S24),IF(AND(L24=\"ดินอ่อน\",O24<=1.5),(((G24+0.2*2)*(H24+0.2*2))*S24),IF(AND(L24=\"ดินแข็ง\",O24<=1.5),(((G24+0.2*2)*(H24+0.2*2))*S24),IF(AND(L24=\"ดินแข็ง\",O24>1.5),(((G24+0.3*2)*(H24+0.3*2))*S24))))),3)","v":0},{"$f":"P24-K24+T24+R24","v":0},"RB 12 mm.","@",null,{"$f":"IF(X24=0,0,((G24/X24)+1)*(H24+(I24*2))*J24)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB24=0,0,((H24/AB24+1)*(G24+I24*2))*J24)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF24=0,0,((I24/AF24+1)*(H24*2+G24*2))*J24)","v":0},{"$f":"(G24*I24*2)+(H24*I24*2)+(D24*F24*2)+(E24*F24*2)","v":0},null,{"$f":"J24*AI24","v":0},null,"RB 12 mm.",{"$f":"IF(F24=0,0,F24+(G24/3))*AK24","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP24=0,0,(ROUNDUP(F24/AP24+1,0)*(D24*2+E24*2))*AK24)","v":0}]
[null,20,"F1-20",0.1,0.1,null,null,null,null,null,{"$f":"(D25*E25*F25+G25*H25*I25)*J25","v":0},"ดินแข็ง",{"$f":"G25","v":0},{"$f":"H25","v":0},null,{"$f":"ROUND(IF(AND(L25=\"ดินแข็ง\",O25<=1.5),((M25+0.2*2)*(N25+0.2*2))*O25,IF(AND(L25=\"ดินแข็ง\",O25>1.5),((M25+0.3*2)+(N25+0.3*2))*O25,IF(AND(O25<=1.5,L25=\"ดินอ่อน\"),1/3*O25*(((N25+0.2*2)*(M25+0.2*2))+((N25+0.3*O25*2)*(M25+0.3*O25*2))+SQRT((((N25+0.2*2)*(M25+0.2*2))*((N25+0.3*O25*2)*(M25+0.3*O25*2))))),IF(AND(O25>1.5,L25=\"ดินอ่อน\"),1/3*O25*(((N25+0.3*2)*(M25+0.3*2))+((N25+0.5*O25*2)*(M25+0.5*O25*2))+SQRT((((N25+0.3*2)*(M25+0.3*2))*((N25+0.5*O25*2)*(M25+0.5*O25*2))))))))),2)*J25","v":0},null,{"$f":"ROUND(IF(AND(L25=\"ดินอ่อน\",O25>1.5),(((G25+0.3*2)*(H25+0.3*2))*Q25),IF(AND(L25=\"ดินอ่อน\",O25<=1.5),(((G25+0.2*2)*(H25+0.2*2))*Q25),IF(AND(L25=\"ดินแข็ง\",O25<=1.5),(((G25+0.2*2)*(H25+0.2*2))*Q25),IF(AND(L25=\"ดินแข็ง\",O25>1.5),(((G25+0.3*2)*(H25+0.3*2))*Q25))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L25=\"ดินอ่อน\",O25>1.5),(((G25+0.3*2)*(H25+0.3*2))*S25),IF(AND(L25=\"ดินอ่อน\",O25<=1.5),(((G25+0.2*2)*(H25+0.2*2))*S25),IF(AND(L25=\"ดินแข็ง\",O25<=1.5),(((G25+0.2*2)*(H25+0.2*2))*S25),IF(AND(L25=\"ดินแข็ง\",O25>1.5),(((G25+0.3*2)*(H25+0.3*2))*S25))))),3)","v":0},{"$f":"P25-K25+T25+R25","v":0},"RB 12 mm.","@",null,{"$f":"IF(X25=0,0,((G25/X25)+1)*(H25+(I25*2))*J25)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB25=0,0,((H25/AB25+1)*(G25+I25*2))*J25)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF25=0,0,((I25/AF25+1)*(H25*2+G25*2))*J25)","v":0},{"$f":"(G25*I25*2)+(H25*I25*2)+(D25*F25*2)+(E25*F25*2)","v":0},null,{"$f":"J25*AI25","v":0},null,"RB 12 mm.",{"$f":"IF(F25=0,0,F25+(G25/3))*AK25","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP25=0,0,(ROUNDUP(F25/AP25+1,0)*(D25*2+E25*2))*AK25)","v":0}]
[null,21,"F1-21",0.1,0.1,null,null,null,null,null,{"$f":"(D26*E26*F26+G26*H26*I26)*J26","v":0},"ดินแข็ง",{"$f":"G26","v":0},{"$f":"H26","v":0},null,{"$f":"ROUND(IF(AND(L26=\"ดินแข็ง\",O26<=1.5),((M26+0.2*2)*(N26+0.2*2))*O26,IF(AND(L26=\"ดินแข็ง\",O26>1.5),((M26+0.3*2)+(N26+0.3*2))*O26,IF(AND(O26<=1.5,L26=\"ดินอ่อน\"),1/3*O26*(((N26+0.2*2)*(M26+0.2*2))+((N26+0.3*O26*2)*(M26+0.3*O26*2))+SQRT((((N26+0.2*2)*(M26+0.2*2))*((N26+0.3*O26*2)*(M26+0.3*O26*2))))),IF(AND(O26>1.5,L26=\"ดินอ่อน\"),1/3*O26*(((N26+0.3*2)*(M26+0.3*2))+((N26+0.5*O26*2)*(M26+0.5*O26*2))+SQRT((((N26+0.3*2)*(M26+0.3*2))*((N26+0.5*O26*2)*(M26+0.5*O26*2))))))))),2)*J26","v":0},null,{"$f":"ROUND(IF(AND(L26=\"ดินอ่อน\",O26>1.5),(((G26+0.3*2)*(H26+0.3*2))*Q26),IF(AND(L26=\"ดินอ่อน\",O26<=1.5),(((G26+0.2*2)*(H26+0.2*2))*Q26),IF(AND(L26=\"ดินแข็ง\",O26<=1.5),(((G26+0.2*2)*(H26+0.2*2))*Q26),IF(AND(L26=\"ดินแข็ง\",O26>1.5),(((G26+0.3*2)*(H26+0.3*2))*Q26))))),3)","v":0},null,{"$f":"ROUND(IF(AND(L26=\"ดินอ่อน\",O26>1.5),(((G26+0.3*2)*(H26+0.3*2))*S26),IF(AND(L26=\"ดินอ่อน\",O26<=1.5),(((G26+0.2*2)*(H26+0.2*2))*S26),IF(AND(L26=\"ดินแข็ง\",O26<=1.5),(((G26+0.2*2)*(H26+0.2*2))*S26),IF(AND(L26=\"ดินแข็ง\",O26>1.5),(((G26+0.3*2)*(H26+0.3*2))*S26))))),3)","v":0},{"$f":"P26-K26+T26+R26","v":0},"RB 12 mm.","@",null,{"$f":"IF(X26=0,0,((G26/X26)+1)*(H26+(I26*2))*J26)","v":0},"DB 12 mm.","@",null,{"$f":"IF(AB26=0,0,((H26/AB26+1)*(G26+I26*2))*J26)","v":0},"RB 15 mm.","@",null,{"$f":"IF(AF26=0,0,((I26/AF26+1)*(H26*2+G26*2))*J26)","v":0},{"$f":"(G26*I26*2)+(H26*I26*2)+(D26*F26*2)+(E26*F26*2)","v":0},null,{"$f":"J26*AI26","v":0},null,"RB 12 mm.",{"$f":"IF(F26=0,0,F26+(G26/3))*AK26","v":0},"DB 12 mm.","@",null,{"$f":"IF(AP26=0,0,(ROUNDUP(F26/AP26+1,0)*(D26*2+E26*2))*AK26)","v":0}]

{"sheet":"รายการคำนวณเสา","index":1,"n_rows":28,"n_cols":20,"rows_kept":28,"cut":false,"hidden":false,"merged":[[0,2,0,3],[4,1,6,2],[4,3,6,3],[5,9,7,9],[5,8,7,8],[6,12,7,12],[4,11,4,19],[6,13,7,13],[6,15,7,15],[5,11,5,13],[5,14,5,16],[5,17,5,18],[5,19,7,19],[5,10,7,10],[6,18,7,18],[6,11,7,11],[5,4,6,7],[4,4,4,9],[6,14,7,14],[6,16,7,16],[6,17,7,17]]}
[null,null,"ประมาณงานเสา"]
[]
[]
[]
[null,"เสาคอนกรีตเสริมเหล็ก",null,"รูปแบบเสา","ปริมาณคอนกรีต",null,null,null,null,null,"งานไม้แบบ","งานเหล็กเสริมเสาคอนกรีต"]
[null,null,null,null,"ขนาดเสา",null,null,null,"จำนวนเสา   ( ต้น )","รวม(m.3)","รวม (m.2)","เหล็กยืน",null,null,"เหล็กปลอกนอก",null,null,"ปลอกเหล็กใน",null," รวมความยาวเหล็กปลอก (m.)"]
[null,null,null,null,null,null,null,null,null,null,null,"ขนาดเหล็กยืน ø (m.)","จำนวนเหล็กยืน (ท่อน)","    รวม     (m.)","เลือกรูปแบบเหล็กปลอก (m.)","ขนาดเหล็กปลอกø  (m.)","ระยะหุ้มคอนกรีต (m.)","ขนาดเหล็กปลอกø  (m.)","ระยะห่างเหล็กปลอก  @  (m.)"]
[null,"ลำดับ","รายการ","choose","r (รัศมี)","b","L","h"]
[null,1,"c1","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D9=\"เสาเหลี่ยม\",F9*G9*H9*I9,((PI()*E9^2)*H9*I9)),3)","v":0},{"$f":"ROUND(IF(D9=\"เสาเหลี่ยม\",((F9*H9*2)+(G9*H9*2))*I9,2*PI()*E9*H9*I9),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L9=\"RB 12 mm.\",L9=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H9)*M9,IF(L9=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H9)*M9,IF(L9=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H9)*M9,IF(L9=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H9)*M9,IF(L9=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H9)*M9,IF(L9=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H9)*M9,IF(L9=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H9)*M9,IF(OR(L9=\"DB 25 mm.\",L9=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H9)*M9,IF(L9=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H9)*M9,IF(L9=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H9)*M9))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S9=0,0,IF(D9=\"เสากลม\",2*PI()*E9*(ROUND(H9/S9,0)+1),IF(O9=\"แบบ 1\",(((F9-Q9*2)*2+(G9-Q9*2)*2)+0.08)*(ROUND(H9/S9,0)+1),IF(O9=\"แบบ 2\",((((F9-Q9*2)*2+(G9-Q9*2)*2)+0.08)+(F9-Q9)*2+0.08)*(ROUND(H9/S9,0)+1),IF(O9=\"แบบ 3\",((((F9-Q9*2)*2+(G9-Q9*2)*2)+0.08+(((F9-Q9*2)/2)+((G9-Q9*2)/2))*2)+0.08)*(ROUND(H9/S9,0)+1),IF(O9=\"แบบ 4\",((((F9-Q9*2)*2+(G9-Q9*2)*2)+0.08)+((F9-Q9*2)+(G9-Q9*2))+0.08+((F9-Q9*2)+(G9-Q9*2))/4)*(ROUND(H9/S9,0)+1),IF(O9=\"แบบ 5\",((((F9-Q9*2)*2+(G9-Q9*2)*2)+0.08)+(((F9-Q9*2)*2+(G9-Q9*2)*2)+0.08)+(1/3*(F9-Q9*2))*2+(1/3*(G9-Q9*2))*2)*(ROUND(H9/S9,0)+1))))))))","v":0}]
[null,2,"c2","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D10=\"เสาเหลี่ยม\",F10*G10*H10*I10,((PI()*E10^2)*H10*I10)),3)","v":0},{"$f":"ROUND(IF(D10=\"เสาเหลี่ยม\",((F10*H10*2)+(G10*H10*2))*I10,2*PI()*E10*H10*I10),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L10=\"RB 12 mm.\",L10=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H10)*M10,IF(L10=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H10)*M10,IF(L10=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H10)*M10,IF(L10=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H10)*M10,IF(L10=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H10)*M10,IF(L10=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H10)*M10,IF(L10=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H10)*M10,IF(OR(L10=\"DB 25 mm.\",L10=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H10)*M10,IF(L10=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H10)*M10,IF(L10=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H10)*M10))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S10=0,0,IF(D10=\"เสากลม\",2*PI()*E10*(ROUND(H10/S10,0)+1),IF(O10=\"แบบ 1\",(((F10-Q10*2)*2+(G10-Q10*2)*2)+0.08)*(ROUND(H10/S10,0)+1),IF(O10=\"แบบ 2\",((((F10-Q10*2)*2+(G10-Q10*2)*2)+0.08)+(F10-Q10)*2+0.08)*(ROUND(H10/S10,0)+1),IF(O10=\"แบบ 3\",((((F10-Q10*2)*2+(G10-Q10*2)*2)+0.08+(((F10-Q10*2)/2)+((G10-Q10*2)/2))*2)+0.08)*(ROUND(H10/S10,0)+1),IF(O10=\"แบบ 4\",((((F10-Q10*2)*2+(G10-Q10*2)*2)+0.08)+((F10-Q10*2)+(G10-Q10*2))+0.08+((F10-Q10*2)+(G10-Q10*2))/4)*(ROUND(H10/S10,0)+1),IF(O10=\"แบบ 5\",((((F10-Q10*2)*2+(G10-Q10*2)*2)+0.08)+(((F10-Q10*2)*2+(G10-Q10*2)*2)+0.08)+(1/3*(F10-Q10*2))*2+(1/3*(G10-Q10*2))*2)*(ROUND(H10/S10,0)+1))))))))","v":0}]
[null,3,"c3","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D11=\"เสาเหลี่ยม\",F11*G11*H11*I11,((PI()*E11^2)*H11*I11)),3)","v":0},{"$f":"ROUND(IF(D11=\"เสาเหลี่ยม\",((F11*H11*2)+(G11*H11*2))*I11,2*PI()*E11*H11*I11),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L11=\"RB 12 mm.\",L11=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H11)*M11,IF(L11=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H11)*M11,IF(L11=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H11)*M11,IF(L11=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H11)*M11,IF(L11=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H11)*M11,IF(L11=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H11)*M11,IF(L11=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H11)*M11,IF(OR(L11=\"DB 25 mm.\",L11=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H11)*M11,IF(L11=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H11)*M11,IF(L11=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H11)*M11))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S11=0,0,IF(D11=\"เสากลม\",2*PI()*E11*(ROUND(H11/S11,0)+1),IF(O11=\"แบบ 1\",(((F11-Q11*2)*2+(G11-Q11*2)*2)+0.08)*(ROUND(H11/S11,0)+1),IF(O11=\"แบบ 2\",((((F11-Q11*2)*2+(G11-Q11*2)*2)+0.08)+(F11-Q11)*2+0.08)*(ROUND(H11/S11,0)+1),IF(O11=\"แบบ 3\",((((F11-Q11*2)*2+(G11-Q11*2)*2)+0.08+(((F11-Q11*2)/2)+((G11-Q11*2)/2))*2)+0.08)*(ROUND(H11/S11,0)+1),IF(O11=\"แบบ 4\",((((F11-Q11*2)*2+(G11-Q11*2)*2)+0.08)+((F11-Q11*2)+(G11-Q11*2))+0.08+((F11-Q11*2)+(G11-Q11*2))/4)*(ROUND(H11/S11,0)+1),IF(O11=\"แบบ 5\",((((F11-Q11*2)*2+(G11-Q11*2)*2)+0.08)+(((F11-Q11*2)*2+(G11-Q11*2)*2)+0.08)+(1/3*(F11-Q11*2))*2+(1/3*(G11-Q11*2))*2)*(ROUND(H11/S11,0)+1))))))))","v":0}]
[null,4,"c4","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D12=\"เสาเหลี่ยม\",F12*G12*H12*I12,((PI()*E12^2)*H12*I12)),3)","v":0},{"$f":"ROUND(IF(D12=\"เสาเหลี่ยม\",((F12*H12*2)+(G12*H12*2))*I12,2*PI()*E12*H12*I12),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L12=\"RB 12 mm.\",L12=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H12)*M12,IF(L12=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H12)*M12,IF(L12=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H12)*M12,IF(L12=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H12)*M12,IF(L12=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H12)*M12,IF(L12=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H12)*M12,IF(L12=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H12)*M12,IF(OR(L12=\"DB 25 mm.\",L12=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H12)*M12,IF(L12=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H12)*M12,IF(L12=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H12)*M12))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S12=0,0,IF(D12=\"เสากลม\",2*PI()*E12*(ROUND(H12/S12,0)+1),IF(O12=\"แบบ 1\",(((F12-Q12*2)*2+(G12-Q12*2)*2)+0.08)*(ROUND(H12/S12,0)+1),IF(O12=\"แบบ 2\",((((F12-Q12*2)*2+(G12-Q12*2)*2)+0.08)+(F12-Q12)*2+0.08)*(ROUND(H12/S12,0)+1),IF(O12=\"แบบ 3\",((((F12-Q12*2)*2+(G12-Q12*2)*2)+0.08+(((F12-Q12*2)/2)+((G12-Q12*2)/2))*2)+0.08)*(ROUND(H12/S12,0)+1),IF(O12=\"แบบ 4\",((((F12-Q12*2)*2+(G12-Q12*2)*2)+0.08)+((F12-Q12*2)+(G12-Q12*2))+0.08+((F12-Q12*2)+(G12-Q12*2))/4)*(ROUND(H12/S12,0)+1),IF(O12=\"แบบ 5\",((((F12-Q12*2)*2+(G12-Q12*2)*2)+0.08)+(((F12-Q12*2)*2+(G12-Q12*2)*2)+0.08)+(1/3*(F12-Q12*2))*2+(1/3*(G12-Q12*2))*2)*(ROUND(H12/S12,0)+1))))))))","v":0}]
[null,5,"c5","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D13=\"เสาเหลี่ยม\",F13*G13*H13*I13,((PI()*E13^2)*H13*I13)),3)","v":0},{"$f":"ROUND(IF(D13=\"เสาเหลี่ยม\",((F13*H13*2)+(G13*H13*2))*I13,2*PI()*E13*H13*I13),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L13=\"RB 12 mm.\",L13=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H13)*M13,IF(L13=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H13)*M13,IF(L13=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H13)*M13,IF(L13=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H13)*M13,IF(L13=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H13)*M13,IF(L13=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H13)*M13,IF(L13=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H13)*M13,IF(OR(L13=\"DB 25 mm.\",L13=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H13)*M13,IF(L13=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H13)*M13,IF(L13=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H13)*M13))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S13=0,0,IF(D13=\"เสากลม\",2*PI()*E13*(ROUND(H13/S13,0)+1),IF(O13=\"แบบ 1\",(((F13-Q13*2)*2+(G13-Q13*2)*2)+0.08)*(ROUND(H13/S13,0)+1),IF(O13=\"แบบ 2\",((((F13-Q13*2)*2+(G13-Q13*2)*2)+0.08)+(F13-Q13)*2+0.08)*(ROUND(H13/S13,0)+1),IF(O13=\"แบบ 3\",((((F13-Q13*2)*2+(G13-Q13*2)*2)+0.08+(((F13-Q13*2)/2)+((G13-Q13*2)/2))*2)+0.08)*(ROUND(H13/S13,0)+1),IF(O13=\"แบบ 4\",((((F13-Q13*2)*2+(G13-Q13*2)*2)+0.08)+((F13-Q13*2)+(G13-Q13*2))+0.08+((F13-Q13*2)+(G13-Q13*2))/4)*(ROUND(H13/S13,0)+1),IF(O13=\"แบบ 5\",((((F13-Q13*2)*2+(G13-Q13*2)*2)+0.08)+(((F13-Q13*2)*2+(G13-Q13*2)*2)+0.08)+(1/3*(F13-Q13*2))*2+(1/3*(G13-Q13*2))*2)*(ROUND(H13/S13,0)+1))))))))","v":0}]
[null,6,"c6","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D14=\"เสาเหลี่ยม\",F14*G14*H14*I14,((PI()*E14^2)*H14*I14)),3)","v":0},{"$f":"ROUND(IF(D14=\"เสาเหลี่ยม\",((F14*H14*2)+(G14*H14*2))*I14,2*PI()*E14*H14*I14),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L14=\"RB 12 mm.\",L14=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H14)*M14,IF(L14=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H14)*M14,IF(L14=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H14)*M14,IF(L14=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H14)*M14,IF(L14=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H14)*M14,IF(L14=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H14)*M14,IF(L14=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H14)*M14,IF(OR(L14=\"DB 25 mm.\",L14=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H14)*M14,IF(L14=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H14)*M14,IF(L14=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H14)*M14))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S14=0,0,IF(D14=\"เสากลม\",2*PI()*E14*(ROUND(H14/S14,0)+1),IF(O14=\"แบบ 1\",(((F14-Q14*2)*2+(G14-Q14*2)*2)+0.08)*(ROUND(H14/S14,0)+1),IF(O14=\"แบบ 2\",((((F14-Q14*2)*2+(G14-Q14*2)*2)+0.08)+(F14-Q14)*2+0.08)*(ROUND(H14/S14,0)+1),IF(O14=\"แบบ 3\",((((F14-Q14*2)*2+(G14-Q14*2)*2)+0.08+(((F14-Q14*2)/2)+((G14-Q14*2)/2))*2)+0.08)*(ROUND(H14/S14,0)+1),IF(O14=\"แบบ 4\",((((F14-Q14*2)*2+(G14-Q14*2)*2)+0.08)+((F14-Q14*2)+(G14-Q14*2))+0.08+((F14-Q14*2)+(G14-Q14*2))/4)*(ROUND(H14/S14,0)+1),IF(O14=\"แบบ 5\",((((F14-Q14*2)*2+(G14-Q14*2)*2)+0.08)+(((F14-Q14*2)*2+(G14-Q14*2)*2)+0.08)+(1/3*(F14-Q14*2))*2+(1/3*(G14-Q14*2))*2)*(ROUND(H14/S14,0)+1))))))))","v":0}]
[null,7,"c7","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D15=\"เสาเหลี่ยม\",F15*G15*H15*I15,((PI()*E15^2)*H15*I15)),3)","v":0},{"$f":"ROUND(IF(D15=\"เสาเหลี่ยม\",((F15*H15*2)+(G15*H15*2))*I15,2*PI()*E15*H15*I15),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L15=\"RB 12 mm.\",L15=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H15)*M15,IF(L15=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H15)*M15,IF(L15=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H15)*M15,IF(L15=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H15)*M15,IF(L15=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H15)*M15,IF(L15=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H15)*M15,IF(L15=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H15)*M15,IF(OR(L15=\"DB 25 mm.\",L15=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H15)*M15,IF(L15=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H15)*M15,IF(L15=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H15)*M15))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S15=0,0,IF(D15=\"เสากลม\",2*PI()*E15*(ROUND(H15/S15,0)+1),IF(O15=\"แบบ 1\",(((F15-Q15*2)*2+(G15-Q15*2)*2)+0.08)*(ROUND(H15/S15,0)+1),IF(O15=\"แบบ 2\",((((F15-Q15*2)*2+(G15-Q15*2)*2)+0.08)+(F15-Q15)*2+0.08)*(ROUND(H15/S15,0)+1),IF(O15=\"แบบ 3\",((((F15-Q15*2)*2+(G15-Q15*2)*2)+0.08+(((F15-Q15*2)/2)+((G15-Q15*2)/2))*2)+0.08)*(ROUND(H15/S15,0)+1),IF(O15=\"แบบ 4\",((((F15-Q15*2)*2+(G15-Q15*2)*2)+0.08)+((F15-Q15*2)+(G15-Q15*2))+0.08+((F15-Q15*2)+(G15-Q15*2))/4)*(ROUND(H15/S15,0)+1),IF(O15=\"แบบ 5\",((((F15-Q15*2)*2+(G15-Q15*2)*2)+0.08)+(((F15-Q15*2)*2+(G15-Q15*2)*2)+0.08)+(1/3*(F15-Q15*2))*2+(1/3*(G15-Q15*2))*2)*(ROUND(H15/S15,0)+1))))))))","v":0}]
[null,8,"c8","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D16=\"เสาเหลี่ยม\",F16*G16*H16*I16,((PI()*E16^2)*H16*I16)),3)","v":0},{"$f":"ROUND(IF(D16=\"เสาเหลี่ยม\",((F16*H16*2)+(G16*H16*2))*I16,2*PI()*E16*H16*I16),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L16=\"RB 12 mm.\",L16=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H16)*M16,IF(L16=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H16)*M16,IF(L16=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H16)*M16,IF(L16=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H16)*M16,IF(L16=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H16)*M16,IF(L16=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H16)*M16,IF(L16=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H16)*M16,IF(OR(L16=\"DB 25 mm.\",L16=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H16)*M16,IF(L16=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H16)*M16,IF(L16=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H16)*M16))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S16=0,0,IF(D16=\"เสากลม\",2*PI()*E16*(ROUND(H16/S16,0)+1),IF(O16=\"แบบ 1\",(((F16-Q16*2)*2+(G16-Q16*2)*2)+0.08)*(ROUND(H16/S16,0)+1),IF(O16=\"แบบ 2\",((((F16-Q16*2)*2+(G16-Q16*2)*2)+0.08)+(F16-Q16)*2+0.08)*(ROUND(H16/S16,0)+1),IF(O16=\"แบบ 3\",((((F16-Q16*2)*2+(G16-Q16*2)*2)+0.08+(((F16-Q16*2)/2)+((G16-Q16*2)/2))*2)+0.08)*(ROUND(H16/S16,0)+1),IF(O16=\"แบบ 4\",((((F16-Q16*2)*2+(G16-Q16*2)*2)+0.08)+((F16-Q16*2)+(G16-Q16*2))+0.08+((F16-Q16*2)+(G16-Q16*2))/4)*(ROUND(H16/S16,0)+1),IF(O16=\"แบบ 5\",((((F16-Q16*2)*2+(G16-Q16*2)*2)+0.08)+(((F16-Q16*2)*2+(G16-Q16*2)*2)+0.08)+(1/3*(F16-Q16*2))*2+(1/3*(G16-Q16*2))*2)*(ROUND(H16/S16,0)+1))))))))","v":0}]
[null,9,"c9","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D17=\"เสาเหลี่ยม\",F17*G17*H17*I17,((PI()*E17^2)*H17*I17)),3)","v":0},{"$f":"ROUND(IF(D17=\"เสาเหลี่ยม\",((F17*H17*2)+(G17*H17*2))*I17,2*PI()*E17*H17*I17),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L17=\"RB 12 mm.\",L17=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H17)*M17,IF(L17=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H17)*M17,IF(L17=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H17)*M17,IF(L17=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H17)*M17,IF(L17=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H17)*M17,IF(L17=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H17)*M17,IF(L17=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H17)*M17,IF(OR(L17=\"DB 25 mm.\",L17=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H17)*M17,IF(L17=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H17)*M17,IF(L17=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H17)*M17))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S17=0,0,IF(D17=\"เสากลม\",2*PI()*E17*(ROUND(H17/S17,0)+1),IF(O17=\"แบบ 1\",(((F17-Q17*2)*2+(G17-Q17*2)*2)+0.08)*(ROUND(H17/S17,0)+1),IF(O17=\"แบบ 2\",((((F17-Q17*2)*2+(G17-Q17*2)*2)+0.08)+(F17-Q17)*2+0.08)*(ROUND(H17/S17,0)+1),IF(O17=\"แบบ 3\",((((F17-Q17*2)*2+(G17-Q17*2)*2)+0.08+(((F17-Q17*2)/2)+((G17-Q17*2)/2))*2)+0.08)*(ROUND(H17/S17,0)+1),IF(O17=\"แบบ 4\",((((F17-Q17*2)*2+(G17-Q17*2)*2)+0.08)+((F17-Q17*2)+(G17-Q17*2))+0.08+((F17-Q17*2)+(G17-Q17*2))/4)*(ROUND(H17/S17,0)+1),IF(O17=\"แบบ 5\",((((F17-Q17*2)*2+(G17-Q17*2)*2)+0.08)+(((F17-Q17*2)*2+(G17-Q17*2)*2)+0.08)+(1/3*(F17-Q17*2))*2+(1/3*(G17-Q17*2))*2)*(ROUND(H17/S17,0)+1))))))))","v":0}]
[null,10,"c10","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D18=\"เสาเหลี่ยม\",F18*G18*H18*I18,((PI()*E18^2)*H18*I18)),3)","v":0},{"$f":"ROUND(IF(D18=\"เสาเหลี่ยม\",((F18*H18*2)+(G18*H18*2))*I18,2*PI()*E18*H18*I18),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L18=\"RB 12 mm.\",L18=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H18)*M18,IF(L18=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H18)*M18,IF(L18=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H18)*M18,IF(L18=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H18)*M18,IF(L18=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H18)*M18,IF(L18=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H18)*M18,IF(L18=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H18)*M18,IF(OR(L18=\"DB 25 mm.\",L18=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H18)*M18,IF(L18=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H18)*M18,IF(L18=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H18)*M18))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S18=0,0,IF(D18=\"เสากลม\",2*PI()*E18*(ROUND(H18/S18,0)+1),IF(O18=\"แบบ 1\",(((F18-Q18*2)*2+(G18-Q18*2)*2)+0.08)*(ROUND(H18/S18,0)+1),IF(O18=\"แบบ 2\",((((F18-Q18*2)*2+(G18-Q18*2)*2)+0.08)+(F18-Q18)*2+0.08)*(ROUND(H18/S18,0)+1),IF(O18=\"แบบ 3\",((((F18-Q18*2)*2+(G18-Q18*2)*2)+0.08+(((F18-Q18*2)/2)+((G18-Q18*2)/2))*2)+0.08)*(ROUND(H18/S18,0)+1),IF(O18=\"แบบ 4\",((((F18-Q18*2)*2+(G18-Q18*2)*2)+0.08)+((F18-Q18*2)+(G18-Q18*2))+0.08+((F18-Q18*2)+(G18-Q18*2))/4)*(ROUND(H18/S18,0)+1),IF(O18=\"แบบ 5\",((((F18-Q18*2)*2+(G18-Q18*2)*2)+0.08)+(((F18-Q18*2)*2+(G18-Q18*2)*2)+0.08)+(1/3*(F18-Q18*2))*2+(1/3*(G18-Q18*2))*2)*(ROUND(H18/S18,0)+1))))))))","v":0}]
[null,11,"c11","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D19=\"เสาเหลี่ยม\",F19*G19*H19*I19,((PI()*E19^2)*H19*I19)),3)","v":0},{"$f":"ROUND(IF(D19=\"เสาเหลี่ยม\",((F19*H19*2)+(G19*H19*2))*I19,2*PI()*E19*H19*I19),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L19=\"RB 12 mm.\",L19=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H19)*M19,IF(L19=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H19)*M19,IF(L19=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H19)*M19,IF(L19=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H19)*M19,IF(L19=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H19)*M19,IF(L19=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H19)*M19,IF(L19=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H19)*M19,IF(OR(L19=\"DB 25 mm.\",L19=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H19)*M19,IF(L19=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H19)*M19,IF(L19=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H19)*M19))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S19=0,0,IF(D19=\"เสากลม\",2*PI()*E19*(ROUND(H19/S19,0)+1),IF(O19=\"แบบ 1\",(((F19-Q19*2)*2+(G19-Q19*2)*2)+0.08)*(ROUND(H19/S19,0)+1),IF(O19=\"แบบ 2\",((((F19-Q19*2)*2+(G19-Q19*2)*2)+0.08)+(F19-Q19)*2+0.08)*(ROUND(H19/S19,0)+1),IF(O19=\"แบบ 3\",((((F19-Q19*2)*2+(G19-Q19*2)*2)+0.08+(((F19-Q19*2)/2)+((G19-Q19*2)/2))*2)+0.08)*(ROUND(H19/S19,0)+1),IF(O19=\"แบบ 4\",((((F19-Q19*2)*2+(G19-Q19*2)*2)+0.08)+((F19-Q19*2)+(G19-Q19*2))+0.08+((F19-Q19*2)+(G19-Q19*2))/4)*(ROUND(H19/S19,0)+1),IF(O19=\"แบบ 5\",((((F19-Q19*2)*2+(G19-Q19*2)*2)+0.08)+(((F19-Q19*2)*2+(G19-Q19*2)*2)+0.08)+(1/3*(F19-Q19*2))*2+(1/3*(G19-Q19*2))*2)*(ROUND(H19/S19,0)+1))))))))","v":0}]
[null,12,"c12","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D20=\"เสาเหลี่ยม\",F20*G20*H20*I20,((PI()*E20^2)*H20*I20)),3)","v":0},{"$f":"ROUND(IF(D20=\"เสาเหลี่ยม\",((F20*H20*2)+(G20*H20*2))*I20,2*PI()*E20*H20*I20),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L20=\"RB 12 mm.\",L20=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H20)*M20,IF(L20=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H20)*M20,IF(L20=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H20)*M20,IF(L20=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H20)*M20,IF(L20=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H20)*M20,IF(L20=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H20)*M20,IF(L20=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H20)*M20,IF(OR(L20=\"DB 25 mm.\",L20=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H20)*M20,IF(L20=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H20)*M20,IF(L20=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H20)*M20))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S20=0,0,IF(D20=\"เสากลม\",2*PI()*E20*(ROUND(H20/S20,0)+1),IF(O20=\"แบบ 1\",(((F20-Q20*2)*2+(G20-Q20*2)*2)+0.08)*(ROUND(H20/S20,0)+1),IF(O20=\"แบบ 2\",((((F20-Q20*2)*2+(G20-Q20*2)*2)+0.08)+(F20-Q20)*2+0.08)*(ROUND(H20/S20,0)+1),IF(O20=\"แบบ 3\",((((F20-Q20*2)*2+(G20-Q20*2)*2)+0.08+(((F20-Q20*2)/2)+((G20-Q20*2)/2))*2)+0.08)*(ROUND(H20/S20,0)+1),IF(O20=\"แบบ 4\",((((F20-Q20*2)*2+(G20-Q20*2)*2)+0.08)+((F20-Q20*2)+(G20-Q20*2))+0.08+((F20-Q20*2)+(G20-Q20*2))/4)*(ROUND(H20/S20,0)+1),IF(O20=\"แบบ 5\",((((F20-Q20*2)*2+(G20-Q20*2)*2)+0.08)+(((F20-Q20*2)*2+(G20-Q20*2)*2)+0.08)+(1/3*(F20-Q20*2))*2+(1/3*(G20-Q20*2))*2)*(ROUND(H20/S20,0)+1))))))))","v":0}]
[null,13,"c13","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D21=\"เสาเหลี่ยม\",F21*G21*H21*I21,((PI()*E21^2)*H21*I21)),3)","v":0},{"$f":"ROUND(IF(D21=\"เสาเหลี่ยม\",((F21*H21*2)+(G21*H21*2))*I21,2*PI()*E21*H21*I21),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L21=\"RB 12 mm.\",L21=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H21)*M21,IF(L21=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H21)*M21,IF(L21=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H21)*M21,IF(L21=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H21)*M21,IF(L21=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H21)*M21,IF(L21=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H21)*M21,IF(L21=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H21)*M21,IF(OR(L21=\"DB 25 mm.\",L21=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H21)*M21,IF(L21=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H21)*M21,IF(L21=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H21)*M21))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S21=0,0,IF(D21=\"เสากลม\",2*PI()*E21*(ROUND(H21/S21,0)+1),IF(O21=\"แบบ 1\",(((F21-Q21*2)*2+(G21-Q21*2)*2)+0.08)*(ROUND(H21/S21,0)+1),IF(O21=\"แบบ 2\",((((F21-Q21*2)*2+(G21-Q21*2)*2)+0.08)+(F21-Q21)*2+0.08)*(ROUND(H21/S21,0)+1),IF(O21=\"แบบ 3\",((((F21-Q21*2)*2+(G21-Q21*2)*2)+0.08+(((F21-Q21*2)/2)+((G21-Q21*2)/2))*2)+0.08)*(ROUND(H21/S21,0)+1),IF(O21=\"แบบ 4\",((((F21-Q21*2)*2+(G21-Q21*2)*2)+0.08)+((F21-Q21*2)+(G21-Q21*2))+0.08+((F21-Q21*2)+(G21-Q21*2))/4)*(ROUND(H21/S21,0)+1),IF(O21=\"แบบ 5\",((((F21-Q21*2)*2+(G21-Q21*2)*2)+0.08)+(((F21-Q21*2)*2+(G21-Q21*2)*2)+0.08)+(1/3*(F21-Q21*2))*2+(1/3*(G21-Q21*2))*2)*(ROUND(H21/S21,0)+1))))))))","v":0}]
[null,14,"c14","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D22=\"เสาเหลี่ยม\",F22*G22*H22*I22,((PI()*E22^2)*H22*I22)),3)","v":0},{"$f":"ROUND(IF(D22=\"เสาเหลี่ยม\",((F22*H22*2)+(G22*H22*2))*I22,2*PI()*E22*H22*I22),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L22=\"RB 12 mm.\",L22=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H22)*M22,IF(L22=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H22)*M22,IF(L22=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H22)*M22,IF(L22=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H22)*M22,IF(L22=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H22)*M22,IF(L22=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H22)*M22,IF(L22=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H22)*M22,IF(OR(L22=\"DB 25 mm.\",L22=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H22)*M22,IF(L22=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H22)*M22,IF(L22=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H22)*M22))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S22=0,0,IF(D22=\"เสากลม\",2*PI()*E22*(ROUND(H22/S22,0)+1),IF(O22=\"แบบ 1\",(((F22-Q22*2)*2+(G22-Q22*2)*2)+0.08)*(ROUND(H22/S22,0)+1),IF(O22=\"แบบ 2\",((((F22-Q22*2)*2+(G22-Q22*2)*2)+0.08)+(F22-Q22)*2+0.08)*(ROUND(H22/S22,0)+1),IF(O22=\"แบบ 3\",((((F22-Q22*2)*2+(G22-Q22*2)*2)+0.08+(((F22-Q22*2)/2)+((G22-Q22*2)/2))*2)+0.08)*(ROUND(H22/S22,0)+1),IF(O22=\"แบบ 4\",((((F22-Q22*2)*2+(G22-Q22*2)*2)+0.08)+((F22-Q22*2)+(G22-Q22*2))+0.08+((F22-Q22*2)+(G22-Q22*2))/4)*(ROUND(H22/S22,0)+1),IF(O22=\"แบบ 5\",((((F22-Q22*2)*2+(G22-Q22*2)*2)+0.08)+(((F22-Q22*2)*2+(G22-Q22*2)*2)+0.08)+(1/3*(F22-Q22*2))*2+(1/3*(G22-Q22*2))*2)*(ROUND(H22/S22,0)+1))))))))","v":0}]
[null,15,"c15","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D23=\"เสาเหลี่ยม\",F23*G23*H23*I23,((PI()*E23^2)*H23*I23)),3)","v":0},{"$f":"ROUND(IF(D23=\"เสาเหลี่ยม\",((F23*H23*2)+(G23*H23*2))*I23,2*PI()*E23*H23*I23),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L23=\"RB 12 mm.\",L23=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H23)*M23,IF(L23=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H23)*M23,IF(L23=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H23)*M23,IF(L23=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H23)*M23,IF(L23=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H23)*M23,IF(L23=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H23)*M23,IF(L23=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H23)*M23,IF(OR(L23=\"DB 25 mm.\",L23=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H23)*M23,IF(L23=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H23)*M23,IF(L23=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H23)*M23))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S23=0,0,IF(D23=\"เสากลม\",2*PI()*E23*(ROUND(H23/S23,0)+1),IF(O23=\"แบบ 1\",(((F23-Q23*2)*2+(G23-Q23*2)*2)+0.08)*(ROUND(H23/S23,0)+1),IF(O23=\"แบบ 2\",((((F23-Q23*2)*2+(G23-Q23*2)*2)+0.08)+(F23-Q23)*2+0.08)*(ROUND(H23/S23,0)+1),IF(O23=\"แบบ 3\",((((F23-Q23*2)*2+(G23-Q23*2)*2)+0.08+(((F23-Q23*2)/2)+((G23-Q23*2)/2))*2)+0.08)*(ROUND(H23/S23,0)+1),IF(O23=\"แบบ 4\",((((F23-Q23*2)*2+(G23-Q23*2)*2)+0.08)+((F23-Q23*2)+(G23-Q23*2))+0.08+((F23-Q23*2)+(G23-Q23*2))/4)*(ROUND(H23/S23,0)+1),IF(O23=\"แบบ 5\",((((F23-Q23*2)*2+(G23-Q23*2)*2)+0.08)+(((F23-Q23*2)*2+(G23-Q23*2)*2)+0.08)+(1/3*(F23-Q23*2))*2+(1/3*(G23-Q23*2))*2)*(ROUND(H23/S23,0)+1))))))))","v":0}]
[null,16,"c16","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D24=\"เสาเหลี่ยม\",F24*G24*H24*I24,((PI()*E24^2)*H24*I24)),3)","v":0},{"$f":"ROUND(IF(D24=\"เสาเหลี่ยม\",((F24*H24*2)+(G24*H24*2))*I24,2*PI()*E24*H24*I24),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L24=\"RB 12 mm.\",L24=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H24)*M24,IF(L24=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H24)*M24,IF(L24=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H24)*M24,IF(L24=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H24)*M24,IF(L24=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H24)*M24,IF(L24=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H24)*M24,IF(L24=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H24)*M24,IF(OR(L24=\"DB 25 mm.\",L24=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H24)*M24,IF(L24=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H24)*M24,IF(L24=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H24)*M24))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S24=0,0,IF(D24=\"เสากลม\",2*PI()*E24*(ROUND(H24/S24,0)+1),IF(O24=\"แบบ 1\",(((F24-Q24*2)*2+(G24-Q24*2)*2)+0.08)*(ROUND(H24/S24,0)+1),IF(O24=\"แบบ 2\",((((F24-Q24*2)*2+(G24-Q24*2)*2)+0.08)+(F24-Q24)*2+0.08)*(ROUND(H24/S24,0)+1),IF(O24=\"แบบ 3\",((((F24-Q24*2)*2+(G24-Q24*2)*2)+0.08+(((F24-Q24*2)/2)+((G24-Q24*2)/2))*2)+0.08)*(ROUND(H24/S24,0)+1),IF(O24=\"แบบ 4\",((((F24-Q24*2)*2+(G24-Q24*2)*2)+0.08)+((F24-Q24*2)+(G24-Q24*2))+0.08+((F24-Q24*2)+(G24-Q24*2))/4)*(ROUND(H24/S24,0)+1),IF(O24=\"แบบ 5\",((((F24-Q24*2)*2+(G24-Q24*2)*2)+0.08)+(((F24-Q24*2)*2+(G24-Q24*2)*2)+0.08)+(1/3*(F24-Q24*2))*2+(1/3*(G24-Q24*2))*2)*(ROUND(H24/S24,0)+1))))))))","v":0}]
[null,17,"c17","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D25=\"เสาเหลี่ยม\",F25*G25*H25*I25,((PI()*E25^2)*H25*I25)),3)","v":0},{"$f":"ROUND(IF(D25=\"เสาเหลี่ยม\",((F25*H25*2)+(G25*H25*2))*I25,2*PI()*E25*H25*I25),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L25=\"RB 12 mm.\",L25=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H25)*M25,IF(L25=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H25)*M25,IF(L25=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H25)*M25,IF(L25=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H25)*M25,IF(L25=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H25)*M25,IF(L25=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H25)*M25,IF(L25=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H25)*M25,IF(OR(L25=\"DB 25 mm.\",L25=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H25)*M25,IF(L25=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H25)*M25,IF(L25=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H25)*M25))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S25=0,0,IF(D25=\"เสากลม\",2*PI()*E25*(ROUND(H25/S25,0)+1),IF(O25=\"แบบ 1\",(((F25-Q25*2)*2+(G25-Q25*2)*2)+0.08)*(ROUND(H25/S25,0)+1),IF(O25=\"แบบ 2\",((((F25-Q25*2)*2+(G25-Q25*2)*2)+0.08)+(F25-Q25)*2+0.08)*(ROUND(H25/S25,0)+1),IF(O25=\"แบบ 3\",((((F25-Q25*2)*2+(G25-Q25*2)*2)+0.08+(((F25-Q25*2)/2)+((G25-Q25*2)/2))*2)+0.08)*(ROUND(H25/S25,0)+1),IF(O25=\"แบบ 4\",((((F25-Q25*2)*2+(G25-Q25*2)*2)+0.08)+((F25-Q25*2)+(G25-Q25*2))+0.08+((F25-Q25*2)+(G25-Q25*2))/4)*(ROUND(H25/S25,0)+1),IF(O25=\"แบบ 5\",((((F25-Q25*2)*2+(G25-Q25*2)*2)+0.08)+(((F25-Q25*2)*2+(G25-Q25*2)*2)+0.08)+(1/3*(F25-Q25*2))*2+(1/3*(G25-Q25*2))*2)*(ROUND(H25/S25,0)+1))))))))","v":0}]
[null,18,"c18","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D26=\"เสาเหลี่ยม\",F26*G26*H26*I26,((PI()*E26^2)*H26*I26)),3)","v":0},{"$f":"ROUND(IF(D26=\"เสาเหลี่ยม\",((F26*H26*2)+(G26*H26*2))*I26,2*PI()*E26*H26*I26),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L26=\"RB 12 mm.\",L26=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H26)*M26,IF(L26=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H26)*M26,IF(L26=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H26)*M26,IF(L26=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H26)*M26,IF(L26=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H26)*M26,IF(L26=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H26)*M26,IF(L26=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H26)*M26,IF(OR(L26=\"DB 25 mm.\",L26=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H26)*M26,IF(L26=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H26)*M26,IF(L26=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H26)*M26))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S26=0,0,IF(D26=\"เสากลม\",2*PI()*E26*(ROUND(H26/S26,0)+1),IF(O26=\"แบบ 1\",(((F26-Q26*2)*2+(G26-Q26*2)*2)+0.08)*(ROUND(H26/S26,0)+1),IF(O26=\"แบบ 2\",((((F26-Q26*2)*2+(G26-Q26*2)*2)+0.08)+(F26-Q26)*2+0.08)*(ROUND(H26/S26,0)+1),IF(O26=\"แบบ 3\",((((F26-Q26*2)*2+(G26-Q26*2)*2)+0.08+(((F26-Q26*2)/2)+((G26-Q26*2)/2))*2)+0.08)*(ROUND(H26/S26,0)+1),IF(O26=\"แบบ 4\",((((F26-Q26*2)*2+(G26-Q26*2)*2)+0.08)+((F26-Q26*2)+(G26-Q26*2))+0.08+((F26-Q26*2)+(G26-Q26*2))/4)*(ROUND(H26/S26,0)+1),IF(O26=\"แบบ 5\",((((F26-Q26*2)*2+(G26-Q26*2)*2)+0.08)+(((F26-Q26*2)*2+(G26-Q26*2)*2)+0.08)+(1/3*(F26-Q26*2))*2+(1/3*(G26-Q26*2))*2)*(ROUND(H26/S26,0)+1))))))))","v":0}]
[null,19,"c19","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D27=\"เสาเหลี่ยม\",F27*G27*H27*I27,((PI()*E27^2)*H27*I27)),3)","v":0},{"$f":"ROUND(IF(D27=\"เสาเหลี่ยม\",((F27*H27*2)+(G27*H27*2))*I27,2*PI()*E27*H27*I27),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L27=\"RB 12 mm.\",L27=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H27)*M27,IF(L27=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H27)*M27,IF(L27=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H27)*M27,IF(L27=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H27)*M27,IF(L27=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H27)*M27,IF(L27=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H27)*M27,IF(L27=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H27)*M27,IF(OR(L27=\"DB 25 mm.\",L27=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H27)*M27,IF(L27=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H27)*M27,IF(L27=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H27)*M27))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S27=0,0,IF(D27=\"เสากลม\",2*PI()*E27*(ROUND(H27/S27,0)+1),IF(O27=\"แบบ 1\",(((F27-Q27*2)*2+(G27-Q27*2)*2)+0.08)*(ROUND(H27/S27,0)+1),IF(O27=\"แบบ 2\",((((F27-Q27*2)*2+(G27-Q27*2)*2)+0.08)+(F27-Q27)*2+0.08)*(ROUND(H27/S27,0)+1),IF(O27=\"แบบ 3\",((((F27-Q27*2)*2+(G27-Q27*2)*2)+0.08+(((F27-Q27*2)/2)+((G27-Q27*2)/2))*2)+0.08)*(ROUND(H27/S27,0)+1),IF(O27=\"แบบ 4\",((((F27-Q27*2)*2+(G27-Q27*2)*2)+0.08)+((F27-Q27*2)+(G27-Q27*2))+0.08+((F27-Q27*2)+(G27-Q27*2))/4)*(ROUND(H27/S27,0)+1),IF(O27=\"แบบ 5\",((((F27-Q27*2)*2+(G27-Q27*2)*2)+0.08)+(((F27-Q27*2)*2+(G27-Q27*2)*2)+0.08)+(1/3*(F27-Q27*2))*2+(1/3*(G27-Q27*2))*2)*(ROUND(H27/S27,0)+1))))))))","v":0}]
[null,20,"c20","เสาเหลี่ยม",0.15,0.2,0.2,2.7,null,{"$f":"ROUND(IF(D28=\"เสาเหลี่ยม\",F28*G28*H28*I28,((PI()*E28^2)*H28*I28)),3)","v":0},{"$f":"ROUND(IF(D28=\"เสาเหลี่ยม\",((F28*H28*2)+(G28*H28*2))*I28,2*PI()*E28*H28*I28),3)","v":0},"RB 9 mm.",null,{"$f":"IF(OR(L28=\"RB 12 mm.\",L28=\"DB 12 mm.\"),((9*0.012*2)+(40*0.012)+H28)*M28,IF(L28=\"RB 9 mm.\",((9*0.009*2)+(40*0.009)+H28)*M28,IF(L28=\"RB 6 mm.\",((9*0.006*2)+(40*0.006)+H28)*M28,IF(L28=\"RB 15 mm.\",((9*0.015*2)+(40*0.015)+H28)*M28,IF(L28=\"RB 19 mm.\",((9*0.019*2)+(40*0.019)+H28)*M28,IF(L28=\"DB 16 mm.\",((9*0.016*2)+(40*0.016)+H28)*M28,IF(L28=\"DB 20 mm.\",((9*0.02*2)+(40*0.02)+H28)*M28,IF(OR(L28=\"DB 25 mm.\",L28=\"RB 25 mm.\"),((9*0.025*2)+(40*0.025)+H28)*M28,IF(L28=\"DB 28 mm.\",((9*0.028*2)+(40*0.028)+H28)*M28,IF(L28=\"DB 32 mm.\",((9*0.032*2)+(40*0.032)+H28)*M28))))))))))","v":0},"choose ","RB 6 mm.",null,"RB 9 mm.",null,{"$f":"IF(S28=0,0,IF(D28=\"เสากลม\",2*PI()*E28*(ROUND(H28/S28,0)+1),IF(O28=\"แบบ 1\",(((F28-Q28*2)*2+(G28-Q28*2)*2)+0.08)*(ROUND(H28/S28,0)+1),IF(O28=\"แบบ 2\",((((F28-Q28*2)*2+(G28-Q28*2)*2)+0.08)+(F28-Q28)*2+0.08)*(ROUND(H28/S28,0)+1),IF(O28=\"แบบ 3\",((((F28-Q28*2)*2+(G28-Q28*2)*2)+0.08+(((F28-Q28*2)/2)+((G28-Q28*2)/2))*2)+0.08)*(ROUND(H28/S28,0)+1),IF(O28=\"แบบ 4\",((((F28-Q28*2)*2+(G28-Q28*2)*2)+0.08)+((F28-Q28*2)+(G28-Q28*2))+0.08+((F28-Q28*2)+(G28-Q28*2))/4)*(ROUND(H28/S28,0)+1),IF(O28=\"แบบ 5\",((((F28-Q28*2)*2+(G28-Q28*2)*2)+0.08)+(((F28-Q28*2)*2+(G28-Q28*2)*2)+0.08)+(1/3*(F28-Q28*2))*2+(1/3*(G28-Q28*2))*2)*(ROUND(H28/S28,0)+1))))))))","v":0}]